IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-04-02T16:37:21"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_1515(x64) - Exporter 2015.0.2016.0512 - Default UI"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "p.wolanin@wxca.pl" of Organization (no name given)
  Owner history of Person "p.wolanin@wxca.pl" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: CENTI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "cz. 02.2 Pawilon Południowy" | phase "PROJEKT WYKONAWCZY"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "WARSZAWA UL. DYMIŃSKA 13, nr ew. działki: - stanowiąca teren zamknięty: 1/1 obręb 7-01-17", "52.2394523620605", "21.8214836120605"
      IFCBUILDINGSTOREY "Rzut sufitu -7.14" | long name "Rzut sufitu -7.14" | elevation -714.
        contains 9 elements
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 30 cm" | object type "Basic Wall:SW1 - żelbet barwiony 30 cm:536629" | names: "Basic Wall:SW1 - żelbet barwiony 30 cm:6936953", "Basic Wall:SW1 - żelbet barwiony 30 cm:6936995", "Basic Wall:SW1 - żelbet barwiony 30 cm:6951477" | material: layers "Basic Wall:SW1 - żelbet barwiony 30 cm" ("Beton Barwiony Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 20 cm" | object type "Basic Wall:SW1 - żelbet barwiony 20 cm:204370" | names: "Basic Wall:SW1 - żelbet barwiony 20 cm:6937356" | material: layers "Basic Wall:SW1 - żelbet barwiony 20 cm" ("Beton Barwiony Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 20 cm" | object type "Basic Wall:SW1 - żelbet barwiony 20 cm:204370" | names: "Basic Wall:SW1 - żelbet barwiony 20 cm:6937904", "Basic Wall:SW1 - żelbet barwiony 20 cm:6953483", "Basic Wall:SW1 - żelbet barwiony 20 cm:6955073" (+2 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 20 cm" ("Beton Barwiony Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
      IFCBUILDINGSTOREY "098 Rzut Piętra -2 rz.-7.15" | long name "098 Rzut Piętra -2 rz.-7.15" | elevation -578.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "obudowa schodów K3" | names: "obudowa schodów K3:obudowa schodów K3:7646398" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing
      IFCBUILDINGSTOREY "090 rz. -380 Szacht Oddym." | long name "090 rz. -380 Szacht Oddym." | elevation -380.
        contains 4 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 50 cm" | object type "Basic Wall:SW1 - żelbet barwiony 50 cm:3277177" | names: "Basic Wall:SW1 - żelbet barwiony 50 cm:644224" | material: layers "Basic Wall:SW1 - żelbet barwiony 50 cm" ("Beton Barwiony Konstrukcja" 50.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 30 cm" | object type "Basic Wall:SW2 - żelbet zwykły 30 cm:4774648" | names: "Basic Wall:SW2 - żelbet zwykły 30 cm:1206656" | material: layers "Basic Wall:SW2 - żelbet zwykły 30 cm" ("Beton Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | object type "Basic Wall:SW2 - żelbet zwykły 20 cm:2377995" | names: "Basic Wall:SW2 - żelbet zwykły 20 cm:1206737" | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 25 cm" | object type "Basic Wall:SW1 - żelbet barwiony 25 cm:4271839" | names: "Basic Wall:SW1 - żelbet barwiony 25 cm:4071230" | material: layers "Basic Wall:SW1 - żelbet barwiony 25 cm" ("Beton Barwiony Konstrukcja" 25.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
      IFCBUILDINGSTOREY "099 rz. -374" | long name "099 rz. -374" | elevation -374.
        contains 15 elements
          2 x IFCSTAIR | object type "Cast-In-Place Stair:Schody Monolityczne 17x26:1936683" | names: "Cast-In-Place Stair:Stair:6940337", "Cast-In-Place Stair:Stair:6958476" | parts: 4 IFCRAILING, 3 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Supports, Other, Identity Data, Graphics, Construction, Calculation Rules
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 30 cm" | object type "Basic Wall:SW1 - żelbet barwiony 30 cm:536629" | names: "Basic Wall:SW1 - żelbet barwiony 30 cm:6951139", "Basic Wall:SW1 - żelbet barwiony 30 cm:6975670" | material: layers "Basic Wall:SW1 - żelbet barwiony 30 cm" ("Beton Barwiony Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 40 cm" | object type "Basic Wall:SW1 - żelbet barwiony 40 cm:221404" | names: "Basic Wall:SW1 - żelbet barwiony 40 cm:6951449" | material: layers "Basic Wall:SW1 - żelbet barwiony 40 cm" ("Beton Barwiony Konstrukcja" 40.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | object type "Basic Wall:SW2 - żelbet zwykły 20 cm:2377995" | names: "Basic Wall:SW2 - żelbet zwykły 20 cm:6951472" | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 30 cm" | object type "Basic Wall:SW2 - żelbet zwykły 30 cm:4774648" | names: "Basic Wall:SW2 - żelbet zwykły 30 cm:6961915" | material: layers "Basic Wall:SW2 - żelbet zwykły 30 cm" ("Beton Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GKF EI-60 - 12,5cm" | object type "Basic Wall:GKF EI-60 - 12,5cm:12329376" | names: "Basic Wall:GKF EI-60 - 12,5cm:12330189", "Basic Wall:GKF EI-60 - 12,5cm:12330265" | material: layers "Basic Wall:GKF EI-60 - 12,5cm" ("Plasterboard" 1.25, "Plasterboard" 1.25, "Welna Mineralna" 7.5, "Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:laminat 0,8 cm" | object type "Basic Wall:laminat 0,8 cm:12349527" | names: "Basic Wall:laminat 0,8 cm:12352887", "Basic Wall:laminat 0,8 cm:12354561", "Basic Wall:laminat 0,8 cm:12354723" | material: layers "Basic Wall:laminat 0,8 cm" ("Gypsum Wall Board" 0.8) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK 2 x 1.25" | object type "Basic Wall:GK 2 x 1.25:12360911" | names: "Basic Wall:GK 2 x 1.25:12362025", "Basic Wall:GK 2 x 1.25:12381278", "Basic Wall:GK 2 x 1.25:12381279" | material: layers "Basic Wall:GK 2 x 1.25" ("Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
      IFCBUILDINGSTOREY "090 rz. -347" | long name "090 rz. -347" | elevation -346.999999999915
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "obudowa schodów" | names: "obudowa schodów K1:obudowa schodów:7632266" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing
      IFCBUILDINGSTOREY "099 rz. -320" | long name "099 rz. -320" | elevation -320.
        contains 18 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:styrodur 20 cm" | object type "Basic Wall:styrodur 20 cm:266315" | names: "Basic Wall:styrodur 20 cm:1982063" | material: layers "Basic Wall:styrodur 20 cm" ("Polistyren Ekstrudowany - izolacja termiczna - do znacznych obciążeń" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 30 cm" | object type "Basic Wall:SW2 - żelbet zwykły 30 cm:4774648" | names: "Basic Wall:SW2 - żelbet zwykły 30 cm:7373150", "Basic Wall:SW2 - żelbet zwykły 30 cm:12428189" | material: layers "Basic Wall:SW2 - żelbet zwykły 30 cm" ("Beton Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7678417" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7679315" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7679481" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7681295" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7685795" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7685798" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7686341" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 15 cm" | object type "Basic Wall:SW2 - żelbet zwykły 15 cm:8443527" | names: "Basic Wall:SW2 - żelbet zwykły 15 cm:8443529", "Basic Wall:SW2 - żelbet zwykły 15 cm:8443530" | material: layers "Basic Wall:SW2 - żelbet zwykły 15 cm" ("Beton Konstrukcja" 15.) | property sets: Constraints, Dimensions, Graphics, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK-C50-2x12,5cm" | object type "Basic Wall:GK-C50-2x12,5cm:12333879" | names: "Basic Wall:GK-C50-2x12,5cm:12317782" | material: layers "Basic Wall:GK-C50-2x12,5cm" ("Plasterboard" 1.25, "Plasterboard" 1.25, "Welna Mineralna" 5.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:laminat 0,8 cm" | object type "Basic Wall:laminat 0,8 cm:12349527" | names: "Basic Wall:laminat 0,8 cm:12321470", "Basic Wall:laminat 0,8 cm:12321471", "Basic Wall:laminat 0,8 cm:12321472" (+1 more) | material: layers "Basic Wall:laminat 0,8 cm" ("Gypsum Wall Board" 0.8) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCBUILDINGELEMENTPROXY | object type "BT BUB BAW SWC" | names: "BT BUB BAW SWC:BT BUB BAW SWC:13841597" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing
      IFCBUILDINGSTOREY "100 rz. 0.00 - Parter" | long name "100 rz. 0.00 - Parter" | elevation 8.48967829369940E-11
        contains 2170 elements
          27 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 40 cm" | object type "Basic Wall:SW1 - żelbet barwiony 40 cm:221404" | names: "Basic Wall:SW1 - żelbet barwiony 40 cm:633864", "Basic Wall:SW1 - żelbet barwiony 40 cm:634013", "Basic Wall:SW1 - żelbet barwiony 40 cm:641900" (+24 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 40 cm" ("Beton Barwiony Konstrukcja" 40.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm" | object type "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:1430568" | names: "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:634979", "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:650002", "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:651946" (+5 more) | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm" ("Beton Barwiony Konstrukcja" 15.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej" | object type "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej:495265" | names: "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej:636498", "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej:638551", "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej:641182" (+4 more) | material: layers "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej" ("Beton Barwiony Konstrukcja" 20., "Folia kubełkowa / szczelina wentylacyjna" 1., "Insulation / Thermal Barriers - Rigid insulation" 19.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          6 x IFCSLAB | object type "Floor:ST2 - Płyta na gruncie - w.wykonczeniowe korekta" | FLOOR | names: "Floor:ST2 - Płyta na gruncie - w.wykonczeniowe korekta:637227", "Floor:ST2 - Płyta na gruncie - w.wykonczeniowe korekta:732424", "Floor:ST2 - Płyta na gruncie - w.wykonczeniowe korekta:732453" (+3 more) | material: layers "Floor:ST2 - Płyta na gruncie - w.wykonczeniowe korekta" ("Posadzka betonowa zbrojona" 15., "Welna Mineralna" 12.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SZ5 - obudowa zewnętrzna wnęk" | object type "Basic Wall:SZ5 - obudowa zewnętrzna wnęk:1430354" | names: "Basic Wall:SZ5 - obudowa zewnętrzna wnęk:639257", "Basic Wall:SZ5 - obudowa zewnętrzna wnęk:639994", "Basic Wall:SZ5 - obudowa zewnętrzna wnęk:640229" (+7 more) | material: layers "Basic Wall:SZ5 - obudowa zewnętrzna wnęk" ("Beton Barwiony Konstrukcja" 15., "Insulation / Thermal Barriers - Rigid insulation" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 25 cm" | object type "Basic Wall:SW1 - żelbet barwiony 25 cm:4271839" | names: "Basic Wall:SW1 - żelbet barwiony 25 cm:640312" | material: layers "Basic Wall:SW1 - żelbet barwiony 25 cm" ("Beton Barwiony Konstrukcja" 25.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 30 cm" | object type "Basic Wall:SW1 - żelbet barwiony 30 cm:536629" | names: "Basic Wall:SW1 - żelbet barwiony 30 cm:640914", "Basic Wall:SW1 - żelbet barwiony 30 cm:672260", "Basic Wall:SW1 - żelbet barwiony 30 cm:675227" (+6 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 30 cm" ("Beton Barwiony Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 30 cm" | object type "Basic Wall:SW2 - żelbet zwykły 30 cm:4774648" | names: "Basic Wall:SW2 - żelbet zwykły 30 cm:641394" | material: layers "Basic Wall:SW2 - żelbet zwykły 30 cm" ("Beton Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 20 cm" | object type "Basic Wall:SW1 - żelbet barwiony 20 cm:204370" | names: "Basic Wall:SW1 - żelbet barwiony 20 cm:673525", "Basic Wall:SW1 - żelbet barwiony 20 cm:673736", "Basic Wall:SW1 - żelbet barwiony 20 cm:1206526" (+13 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 20 cm" ("Beton Barwiony Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 KT" | object type "1100 x 2100 KT" | names: "Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100 KT:677092", "Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100 KT:677296" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1200 x 2100" | object type "1200 x 2100" | names: "Drzwi drewniane 1skrz blokowe supraporta 2str:1200 x 2100:677229" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1200 x 2400 brąz" | object type "1200 x 2400 brąz" | names: "Drzwi stalowe 1skrz blokowe:1200 x 2400 brąz:677510" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Metal - Bronze") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | object type "Basic Wall:SW2 - żelbet zwykły 20 cm:2377995" | names: "Basic Wall:SW2 - żelbet zwykły 20 cm:678932", "Basic Wall:SW2 - żelbet zwykły 20 cm:1462371", "Basic Wall:SW2 - żelbet zwykły 20 cm:1462376" (+7 more) | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          6 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami" | object type "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami:290005" | names: "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami:729535", "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami:972720", "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami:973355" (+3 more) | parts: 114 IFCMEMBER, 36 IFCWALLSTANDARDCASE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          2 x IFCSLAB | object type "Floor:ST1 - Płyta na gruncie - w.wykonczeniowe korekta" | FLOOR | names: "Floor:ST1 - Płyta na gruncie - w.wykonczeniowe korekta:732481", "Floor:ST1 - Płyta na gruncie - w.wykonczeniowe korekta:777759" | material: layers "Floor:ST1 - Płyta na gruncie - w.wykonczeniowe korekta" ("Posadzka betonowa zbrojona" 20., "Welna Mineralna" 12.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK4 - Sciana kurtynowa wnętrza pusta" | object type "Curtain Wall:SK4 - Sciana kurtynowa wnętrza pusta:2476880" | names: "Curtain Wall:SK4 - Sciana kurtynowa wnętrza pusta:733247", "Curtain Wall:SK4 - Sciana kurtynowa wnętrza pusta:7120372" | parts: 16 IFCMEMBER, 8 IFCWALLSTANDARDCASE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 70cm" | object type "Basic Wall:SW1 - żelbet barwiony 70cm:3410152" | names: "Basic Wall:SW1 - żelbet barwiony 70cm:1205896", "Basic Wall:SW1 - żelbet barwiony 70cm:1206159" | material: layers "Basic Wall:SW1 - żelbet barwiony 70cm" ("Beton Barwiony Konstrukcja" 70.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 30 cm" | object type "Basic Wall:SW1 - żelbet barwiony 30 cm:536629" | names: "Basic Wall:SW1 - żelbet barwiony 30 cm:1206381" | material: layers "Basic Wall:SW1 - żelbet barwiony 30 cm" ("Beton Barwiony Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:203146" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:1207380", "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:1462370", "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:2071842" (+6 more) | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" ("SILKA" 18.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100" | object type "1100 x 2100" | names: "Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100:1462375" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Materials and Finishes
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW3 - bloczki betonowe 18 cm" | object type "Basic Wall:SW3 - bloczki betonowe 18 cm:4445077" | names: "Basic Wall:SW3 - bloczki betonowe 18 cm:1462377", "Basic Wall:SW3 - bloczki betonowe 18 cm:1462381", "Basic Wall:SW3 - bloczki betonowe 18 cm:1463465" (+2 more) | material: layers "Basic Wall:SW3 - bloczki betonowe 18 cm" ("Beton bloczki" 18.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100" | object type "1100 x 2100" | names: "Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100:1462378" | material: materials ("Door - Frame", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Construction, Dimensions, Identity Data, Materials and Finishes
          1 x IFCSTAIR | object type "Cast-In-Place Stair:Schody Monolityczne 17x26:1936683" | names: "Cast-In-Place Stair:Stair:1486248" | parts: 3 IFCRAILING, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_StairCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCCOVERING | object type "Compound Ceiling:SGK" | CEILING | names: "Compound Ceiling:SGK:1620929" | material: layers "Compound Ceiling:SGK" ("Default" 3.6, "Ceiling Tile 600 x 1200" 1.6) | property sets: Pset_CoveringCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCCOVERING | object type "Compound Ceiling:SGKh" | CEILING | names: "Compound Ceiling:SGKh:1620980" | material: layers "Compound Ceiling:SGKh" ("Default" 3.6, "Ceiling Tile 600 x 1200" 1.6) | property sets: Pset_CoveringCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCCOVERING | object type "Compound Ceiling:SAK 1" | CEILING | names: "Compound Ceiling:SAK 1:1621024", "Compound Ceiling:SAK 1:4982355", "Compound Ceiling:SAK 1:4986852" (+1 more) | material: layers "Compound Ceiling:SAK 1" ("Welna Mineralna" 4., "Plaster" 1.) | property sets: Pset_CoveringCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCCOVERING | object type "Compound Ceiling:SKA (60x60 cm)" | CEILING | names: "Compound Ceiling:SKA (60x60 cm):1621076", "Compound Ceiling:SKA (60x60 cm):3399224", "Compound Ceiling:SKA (60x60 cm):5308480" (+3 more) | material: layers "Compound Ceiling:SKA (60x60 cm)" ("Default transparent" 3.6, "Ceiling Tile 600 x 600" 1.6) | property sets: Pset_CoveringCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCWALL | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:203146" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:2078326", "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:3271867", "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:3272378" (+3 more) | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" ("SILKA" 18.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 40 cm" | object type "Basic Wall:SW2 - żelbet zwykły 40 cm:4583798" | names: "Basic Wall:SW2 - żelbet zwykły 40 cm:2081300" | material: layers "Basic Wall:SW2 - żelbet zwykły 40 cm" ("Beton Konstrukcja" 40.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:ścianka instalacyjna 13 cm" | object type "Basic Wall:ścianka instalacyjna 13 cm:2391863" | names: "Basic Wall:ścianka instalacyjna 13 cm:2391821", "Basic Wall:ścianka instalacyjna 13 cm:2391962", "Basic Wall:ścianka instalacyjna 13 cm:2392077" (+4 more) | material: layers "Basic Wall:ścianka instalacyjna 13 cm" ("Default New Material Konstrukcja" 13.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:ścianka instalacyjna 25 cm" | object type "Basic Wall:ścianka instalacyjna 25 cm:2392242" | names: "Basic Wall:ścianka instalacyjna 25 cm:2392222", "Basic Wall:ścianka instalacyjna 25 cm:2398644", "Basic Wall:ścianka instalacyjna 25 cm:2398645" (+2 more) | material: layers "Basic Wall:ścianka instalacyjna 25 cm" ("Default New Material Konstrukcja" 25.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "40 x 40 cm" | object type "40 x 40 cm" | names: "M_Round Column:40 x 40 cm:2415945", "M_Round Column:40 x 40 cm:2417072", "M_Round Column:40 x 40 cm:2417102" (+3 more) | property sets: Pset_ColumnCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCSLAB | object type "Floor:S0 - Płyty Placu Gwardii 120 x 120" | FLOOR | names: "Floor:S0 - Płyty Placu Gwardii 120 x 120:2524159", "Floor:S0 - Płyty Placu Gwardii 120 x 120:2524159:2", "Floor:S0 - Płyty Placu Gwardii 120 x 120:2524159:3" (+3 more) | material: layers "Floor:S0 - Płyty Placu Gwardii 120 x 120" ("Płyty Placu Gwardii" 10.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          8 x IFCSLAB | object type "Floor:ST - Płyta na gruncie - płyta żelbetowa korekta 18 cm" | FLOOR | names: "Floor:ST - Płyta na gruncie - płyta żelbetowa korekta 18 cm:2530292", "Floor:ST - Płyta na gruncie - płyta żelbetowa korekta 18 cm:3277304", "Floor:ST - Płyta na gruncie - płyta żelbetowa korekta 18 cm:3277304:2" (+5 more) | material: layers "Floor:ST - Płyta na gruncie - płyta żelbetowa korekta 18 cm" ("Beton Konstrukcja" 18.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "1200 x 2400 beton EI-30" | object type "1200 x 2400 beton EI-30" | names: "Drzwi stalowe 1skrz blokowe:1200 x 2400 beton EI-30:2620844" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2" | object type "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2:249111" | names: "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2:2697788", "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2:8394130" | parts: 14 IFCMEMBER, 4 IFCWALLSTANDARDCASE, 1 IFCOPENINGELEMENT | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 Ra32 KD2" | object type "1100 x 2100 Ra32 KD2" | names: "Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra32 KD2:2849913" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 Ra27" | object type "1100 x 2100 Ra27" | names: "Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra27:3273618", "Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra27:9760137" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 blokada wc" | object type "1100 x 2100 blokada wc" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:3273632" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm:203147" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm:3274279", "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm:3274389" | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm" ("SILKA" 8.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100" | object type "1100 x 2100" | names: "Drzwi drewniane 1skrz blokowe supraporta 1str:1100 x 2100:3276145", "Drzwi drewniane 1skrz blokowe supraporta 1str:1100 x 2100:3350677" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          6 x IFCSLAB | object type "Floor:ST3 - Płyta na gruncie - w.wykonczeniowe korekta" | FLOOR | names: "Floor:ST3 - Płyta na gruncie - w.wykonczeniowe korekta:3389151", "Floor:ST3 - Płyta na gruncie - w.wykonczeniowe korekta:3389151:2", "Floor:ST3 - Płyta na gruncie - w.wykonczeniowe korekta:3389151:3" (+3 more) | material: layers "Floor:ST3 - Płyta na gruncie - w.wykonczeniowe korekta" ("Posadzka betonowa zbrojona" 15., "Welna Mineralna" 12.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 Ra32 KD2" | object type "1100 x 2100 Ra32 KD2" | names: "Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra32 KD2:3389960" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 40 cm" | object type "Basic Wall:SW1 - żelbet barwiony 40 cm:221404" | names: "Basic Wall:SW1 - żelbet barwiony 40 cm:3413112" | material: layers "Basic Wall:SW1 - żelbet barwiony 40 cm" ("Beton Barwiony Konstrukcja" 40.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW8 - okładzina SWC" | object type "Basic Wall:SW8 - okładzina SWC:3873135" | names: "Basic Wall:SW8 - okładzina SWC:3873133", "Basic Wall:SW8 - okładzina SWC:3873176", "Basic Wall:SW8 - okładzina SWC:4243907" (+1 more) | material: layers "Basic Wall:SW8 - okładzina SWC" ("Copper z podziałem" 5., "Welna Mineralna Akustyka" 15.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          24 x IFCANNOTATION
          1 x IFCSLAB | object type "Floor:ST - Płyta na gruncie - płyta żelbetowa" | FLOOR | names: "Floor:ST - Płyta na gruncie - płyta żelbetowa:4025878" | material: layers "Floor:ST - Płyta na gruncie - płyta żelbetowa" ("Beton Konstrukcja" 20.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCSLAB | object type "Floor:ST7 - Strop między piętrami - konstrukcja" | FLOOR | names: "Floor:ST7 - Strop między piętrami - konstrukcja:4041478" | material: layers "Floor:ST7 - Strop między piętrami - konstrukcja" ("Beton Konstrukcja" 25.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCSLAB | object type "Floor:ST7 - Strop między piętrami - w.wykonczeniowe" | FLOOR | names: "Floor:ST7 - Strop między piętrami - w.wykonczeniowe:4041589", "Floor:ST7 - Strop między piętrami - w.wykonczeniowe:6942098" | material: layers "Floor:ST7 - Strop między piętrami - w.wykonczeniowe" ("Posadzka - wylewka betonowa" 7., "Styropian EPS - podłoga" 5.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "1900 x 2400 (podział 110 80) ap beton poprawione" | object type "1900 x 2400 (podział 110 80) ap beton poprawione" | names: "Drzwi stalowe 2skrz niesym blokowe:1900 x 2400 (podział 110 80) ap beton poprawione:4071345" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Beton Barwiony Konstrukcja") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          12 x IFCBUILDINGELEMENTPROXY | object type "PORTAL_01" | names: "PORTAL:PORTAL_01:4174309", "PORTAL:PORTAL_01:4175604", "PORTAL:PORTAL_01:4176228" (+9 more) | material: "Metal - Bronze" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCBUILDINGELEMENTPROXY | object type "PORTAL_02 LEWY" | names: "PORTAL_NAROŻNY:PORTAL_02 LEWY:4185181", "PORTAL_NAROŻNY:PORTAL_02 LEWY:4189163" | material: "Metal - Bronze" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCBUILDINGELEMENTPROXY | object type "PORTAL_02 PRAWY" | names: "PORTAL_NAROŻNY:PORTAL_02 PRAWY:4185229", "PORTAL_NAROŻNY:PORTAL_02 PRAWY:4189261" | material: "Metal - Bronze" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:wełna minerlana 12 cm" | object type "Basic Wall:wełna minerlana 12 cm:8395562" | names: "Basic Wall:wełna minerlana 12 cm:4269502", "Basic Wall:wełna minerlana 12 cm:4269932", "Basic Wall:wełna minerlana 12 cm:4270067" (+1 more) | material: layers "Basic Wall:wełna minerlana 12 cm" ("Insulation / Thermal Barriers - Rigid insulation" 12.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK5_Podkonstrukcja" | object type "Curtain Wall:SK5_Podkonstrukcja:4300410" | names: "Curtain Wall:SK5_Podkonstrukcja:4300393" | parts: 17 IFCMEMBER | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.)" | object type "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.):4304849" | names: "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.):4305322", "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.):4305722", "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.):4305843" (+15 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.)" ("Beton Barwiony Okladzina" 3.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          9 x IFCBUILDINGELEMENTPROXY | object type "DN 25 wysuwany" | names: "hydrant:DN 25 wysuwany:4642936", "hydrant:DN 25 wysuwany:4643049", "hydrant:DN 25 wysuwany:4643226" (+6 more) | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCBUILDINGELEMENTPROXY | object type "DN 25 plus ROP" | names: "szafka hydrant + ROP:DN 25 plus ROP:4644950", "szafka hydrant + ROP:DN 25 plus ROP:4645061", "szafka hydrant + ROP:DN 25 plus ROP:4645180" (+1 more) | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza" | object type "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:4895782" | names: "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:4907542", "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:9762795" | parts: 6 IFCMEMBER, 2 IFCWALLSTANDARDCASE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:3295308" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:5174014", "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:5174044", "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:6859626" (+2 more) | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm" ("SILKA" 12.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          3 x IFCCOVERING | object type "Compound Ceiling:SKA (210x60 cm)" | CEILING | names: "Compound Ceiling:SKA (210x60 cm):5308785", "Compound Ceiling:SKA (210x60 cm):5308836", "Compound Ceiling:SKA (210x60 cm):5308882" | material: layers "Compound Ceiling:SKA (210x60 cm)" ("Default transparent" 3.6, "Ceiling Tile 600 x 600(1)" 1.6) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_CoveringCommon
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 183 mm" | object type "Pleiad Comfort G3 183 mm" | names: "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5321879", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5321905", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5321906" (+17 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 183 mm" | object type "Pleiad Comfort G3 183 mm" | names: "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5321931", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5321937", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5321940" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          20 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "TRIL 20.1030.35 116mm" | object type "TRIL 20.1030.35 116mm" | names: "MWP_M_Downlight - Recessed Can:TRIL 20.1030.35 116mm:5321951", "MWP_M_Downlight - Recessed Can:TRIL 20.1030.35 116mm:5321955", "MWP_M_Downlight - Recessed Can:TRIL 20.1030.35 116mm:5321958" (+17 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          19 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 183 mm" | object type "Pleiad Comfort G3 183 mm" | names: "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5368829", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5368831", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 183 mm:5368832" (+16 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          17 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 110 mm" | object type "Pleiad Comfort G3 110 mm" | names: "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 110 mm:5368844", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 110 mm:5368846", "MWP_M_Downlight - Recessed Can:Pleiad Comfort G3 110 mm:5368848" (+14 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          12 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "Pozzo Delta 550mm" | object type "Pozzo Delta 550mm" | names: "MWP_M_Downlight - Recessed Can:Pozzo Delta 550mm:5397393", "MWP_M_Downlight - Recessed Can:Pozzo Delta 550mm:5397658", "MWP_M_Downlight - Recessed Can:Pozzo Delta 550mm:5397846" (+9 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          16 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "CSALP TRI 60.1041.15 143mm" | object type "CSALP TRI 60.1041.15 143mm" | names: "MWP_M_Downlight - Recessed Can:CSALP TRI 60.1041.15 143mm:5449837", "MWP_M_Downlight - Recessed Can:CSALP TRI 60.1041.15 143mm:5450689", "MWP_M_Downlight - Recessed Can:CSALP TRI 60.1041.15 143mm:5450881" (+13 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Surface Lamp PLEIAD G3 180 mm" | object type "MWP_M_Surface Lamp PLEIAD G3 180 mm" | names: "MWP_M_Surface Lamp round:MWP_M_Surface Lamp PLEIAD G3 180 mm:5667571" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCBEAM | object type "HEB:HEB_120x120:5678879" | names: "HEB:HEB_120x120:5679921" | material: "Stal, 45-345" | property sets: Structural, Other, Identity Data, Dimensions, Pset_BeamCommon, Constraints
          2 x IFCBUILDINGELEMENTPROXY | object type "wpust 20 x 20 cm" | names: "wpust podłogowy:wpust 20 x 20 cm:5691065", "wpust podłogowy:wpust 20 x 20 cm:5691066" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:laminat 3cm" | object type "Basic Wall:laminat 3cm:5958839" | names: "Basic Wall:laminat 3cm:5958816", "Basic Wall:laminat 3cm:5958936", "Basic Wall:laminat 3cm:6863466" (+4 more) | material: layers "Basic Wall:laminat 3cm" ("Gypsum Wall Board" 3.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCBUILDINGELEMENTPROXY | object type "grzejnik 3" | names: "grzejnik 3:grzejnik 3:6677024" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing
          2 x IFCSLAB | object type "Floor:ST8 - Strop, żelbet 25 cm" | FLOOR | names: "Floor:ST8 - Strop, żelbet 25 cm:6942157", "Floor:ST8 - Strop, żelbet 25 cm:6942157:2" | material: layers "Floor:ST8 - Strop, żelbet 25 cm" ("Beton Konstrukcja" 25.) | property sets: Other, Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties
          1 x IFCDOOR | type IFCDOORSTYLE "1900 x 2400 mm (podział 110 80) EI-30 ap beton poprawione" | object type "1900 x 2400 mm (podział 110 80) EI-30 ap beton poprawione" | names: "Drzwi stalowe 2skrz niesym blokowe:1900 x 2400 mm (podział 110 80) EI-30 ap beton poprawione:7117541" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Beton Barwiony Okladzina") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW6 - okł. miedziana SWC 5 cm" | object type "Basic Wall:SW6 - okł. miedziana SWC 5 cm:3893706" | names: "Basic Wall:SW6 - okł. miedziana SWC 5 cm:7121344", "Basic Wall:SW6 - okł. miedziana SWC 5 cm:7121595", "Basic Wall:SW6 - okł. miedziana SWC 5 cm:7122048" (+5 more) | material: layers "Basic Wall:SW6 - okł. miedziana SWC 5 cm" ("Copper bez podziału" 5.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy" | object type "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy:9645974" | names: "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy:7122320", "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy:7122677", "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy:7123468" (+1 more) | material: layers "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy" ("Copper bez podziału" 5.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW3 - bloczki betonowe 20 cm" | object type "Basic Wall:SW3 - bloczki betonowe 20 cm:10011253" | names: "Basic Wall:SW3 - bloczki betonowe 20 cm:7122520", "Basic Wall:SW3 - bloczki betonowe 20 cm:9775500" | material: layers "Basic Wall:SW3 - bloczki betonowe 20 cm" ("Beton bloczki" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1175 x 2400 + 4800 sp" | object type "1175 x 2400 + 4800 sp" | names: "Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7133277" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1175 x 2400 + 4800 sp" | object type "1175 x 2400 + 4800 sp" | names: "Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7137746" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1175 x 2400 + 4800 sp" | object type "1175 x 2400 + 4800 sp" | names: "Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7137829" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1175 x 2400 + 4800 sp" | object type "1175 x 2400 + 4800 sp" | names: "Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7138385" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "3275 x 7150 + 50 sp" | object type "3275 x 7150 + 50 sp" | names: "Drzwi indywidualne SWC blokowe:3275 x 7150 + 50 sp:7138557" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCBUILDINGELEMENTPROXY | object type "DN 25 plus ROP SWC" | names: "szafka hydrant + ROP:DN 25 plus ROP SWC:7278543", "szafka hydrant + ROP:DN 25 plus ROP SWC:7278855" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          10 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7618455", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7621387", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7621405" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7621393", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7621411" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7621399" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          6 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Surface Lamp Kaptur LITE 600mm" | object type "MWP_M_Surface Lamp Kaptur LITE 600mm" | names: "MWP_M_Surface Lamp rectangle:MWP_M_Surface Lamp Kaptur LITE 600mm:7630867", "MWP_M_Surface Lamp rectangle:MWP_M_Surface Lamp Kaptur LITE 600mm:7630869", "MWP_M_Surface Lamp rectangle:MWP_M_Surface Lamp Kaptur LITE 600mm:7630870" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7640857" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7641032" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7679172" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          4 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "szynoprzewod" | object type "szynoprzewod" | names: "szynoprzewod:szynoprzewod:7691645", "szynoprzewod:szynoprzewod:8195015", "szynoprzewod:szynoprzewod:8195216" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "szynoprzewod" | object type "szynoprzewod" | names: "szynoprzewod:szynoprzewod:7693598" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "szynoprzewod" | object type "szynoprzewod" | names: "szynoprzewod:szynoprzewod:7693955" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          6 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "TRIL 20.1030.35 116mm" | object type "TRIL 20.1030.35 116mm" | names: "MWP_M_Downlight - Recessed Can:TRIL 20.1030.35 116mm:7694219", "MWP_M_Downlight - Recessed Can:TRIL 20.1030.35 116mm:7694906", "MWP_M_Downlight - Recessed Can:TRIL 20.1030.35 116mm:7694918" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          6 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7888606", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7888716", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900802" (+3 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          11 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7888699", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7888748", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900772" (+8 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7888800" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:laminat 0,8 cm" | object type "Basic Wall:laminat 0,8 cm:12349527" | names: "Basic Wall:laminat 0,8 cm:7892002", "Basic Wall:laminat 0,8 cm:12320759", "Basic Wall:laminat 0,8 cm:12320883" (+5 more) | material: layers "Basic Wall:laminat 0,8 cm" ("Gypsum Wall Board" 0.8) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2400 (beton)" | object type "1100 x 2400 (beton)" | names: "Drzwi stalowe 1skrz blokowe:1100 x 2400 (beton):7898971" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Beton Barwiony Okladzina") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900815" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          157 x IFCBUILDINGELEMENTPROXY | object type "Floorbox 20 x 20 cm" | names: "Floorbox kwadratowy:Floorbox 20 x 20 cm:7919734", "Floorbox kwadratowy:Floorbox 20 x 20 cm:7920028", "Floorbox kwadratowy:Floorbox 20 x 20 cm:7920063" (+154 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          279 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "TRIL 20.1030.25 116mm" | object type "TRIL 20.1030.25 116mm" | names: "MWP_M_Downlight - Recessed Can:TRIL 20.1030.25 116mm:8025879", "MWP_M_Downlight - Recessed Can:TRIL 20.1030.25 116mm:8025880", "MWP_M_Downlight - Recessed Can:TRIL 20.1030.25 116mm:8025881" (+276 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          4 x IFCBUILDINGELEMENTPROXY | object type "Otwór 120 x 40 cm" | names: "Otwór pod projektor:Otwór 120 x 40 cm:8080320", "Otwór pod projektor:Otwór 120 x 40 cm:8080401", "Otwór pod projektor:Otwór 120 x 40 cm:8080429" (+1 more) | material: "Metal - Bronze" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Materials and Finishes
          1 x IFCBUILDINGELEMENTPROXY | object type "Otwór 60 x 40 cm" | names: "Otwór pod projektor:Otwór 60 x 40 cm:8080445" | material: "Metal - Bronze" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Materials and Finishes
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8091177" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8091293", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8091338" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8091312" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK 3cm" | object type "Basic Wall:GK 3cm:8093067" | names: "Basic Wall:GK 3cm:8120447", "Basic Wall:GK 3cm:8213552", "Basic Wall:GK 3cm:8213553" (+6 more) | material: layers "Basic Wall:GK 3cm" ("Gypsum Wall Board" 3.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "szynoprzewod" | object type "szynoprzewod" | names: "szynoprzewod:szynoprzewod:8196180" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8211936", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8211937", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8211939" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          3 x IFCSLAB | object type "Floor:SK - płyta gk" | FLOOR | names: "Floor:SK - płyta gk:8213558", "Floor:SK - płyta gk:8213558:2", "Floor:SK - płyta gk:8213558:3" | material: layers "Floor:SK - płyta gk" ("Gypsum Wall Board" 5.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCSLAB | object type "Floor:S3 - strop żelbet 12 cm" | FLOOR | names: "Floor:S3 - strop żelbet 12 cm:8213585" | material: layers "Floor:S3 - strop żelbet 12 cm" ("Beton Konstrukcja" 12.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK wełna GK" | object type "Basic Wall:GK wełna GK:8213619" | names: "Basic Wall:GK wełna GK:8213617" | material: layers "Basic Wall:GK wełna GK" ("Gypsum Wall Board" 1.25, "Insulation / Thermal Barriers - Rigid insulation" 7., "Gypsum Wall Board" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 9 wc" | object type "LK 005.1 AG/ 9 wc" | names: "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 9 wc:8298130" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 9 wc" | object type "LK 005.1 AG/ 9 wc" | names: "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 9 wc:8299992" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCSLAB | object type "Floor:S0 - Fundament 15 cm" | FLOOR | names: "Floor:S0 - Fundament 15 cm:8443594" | material: layers "Floor:S0 - Fundament 15 cm" ("Beton Konstrukcja" 15.) | property sets: Other, Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties
          1 x IFCBUILDINGELEMENTPROXY | object type "60 x 60 cm" | names: "Właz podłogowy:60 x 60 cm:8458859" | material: "Posadzka betonowa zbrojona" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Materials and Finishes
          1 x IFCCOVERING | object type "Compound Ceiling:SUFIT SBAG" | CEILING | names: "Compound Ceiling:SUFIT SBAG:8511302" | material: layers "Compound Ceiling:SUFIT SBAG" ("Beton Barwiony Konstrukcja" 15.) | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_CoveringCommon
          46 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" | object type "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" | names: "MWP_M_Downlight - Recessed Can:MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90:8511434", "MWP_M_Downlight - Recessed Can:MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90:8511495", "MWP_M_Downlight - Recessed Can:MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90:8511497" (+43 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" | object type "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" | names: "MWP_M_Downlight - Recessed Can:MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90:8511496" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Circuiting, Electrical - Lighting, Electrical - Loads
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100" | object type "1100 x 2100" | names: "Drzwi stalowe 1skrz blokowe:1100 x 2100:8563773" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCBUILDINGELEMENTPROXY | object type "Generic Models 1" | names: "Generic Models 1:Generic Models 1:8569216", "Generic Models 2:Generic Models 1:8569332" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Phasing
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:wełna minerlana 15 cm" | object type "Basic Wall:wełna minerlana 15 cm:8578302" | names: "Basic Wall:wełna minerlana 15 cm:8578241", "Basic Wall:wełna minerlana 15 cm:8578563", "Basic Wall:wełna minerlana 15 cm:8579008" (+8 more) | material: layers "Basic Wall:wełna minerlana 15 cm" ("Insulation / Thermal Barriers - Rigid insulation" 15.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          335 x IFCBUILDINGELEMENTPROXY | object type "260 x 260 cm" | names: "Domknięcie akustyki:260 x 260 cm:8799265", "Domknięcie akustyki:260 x 260 cm:8799266", "Domknięcie akustyki:260 x 260 cm:8799267" (+332 more) | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          130 x IFCBUILDINGELEMENTPROXY | object type "360 x 130 cm" | names: "Domknięcie akustyki:360 x 130 cm:8803839", "Domknięcie akustyki:360 x 130 cm:8807677", "Domknięcie akustyki:360 x 130 cm:8808337" (+127 more) | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          8 x IFCBUILDINGELEMENTPROXY | object type "220 x 130 cm" | names: "Domknięcie akustyki:220 x 130 cm:8809497", "Domknięcie akustyki:220 x 130 cm:8812146", "Domknięcie akustyki:220 x 130 cm:8812278" (+5 more) | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          10 x IFCBUILDINGELEMENTPROXY | object type "360 x 150 cm" | names: "Domknięcie akustyki:360 x 150 cm:8810023", "Domknięcie akustyki:360 x 150 cm:8810024", "Domknięcie akustyki:360 x 150 cm:8810025" (+7 more) | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          1 x IFCBUILDINGELEMENTPROXY | object type "360 x 320 cm" | names: "Domknięcie akustyki:360 x 320 cm:8811561" | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          8 x IFCBUILDINGELEMENTPROXY | object type "220 x 150 cm" | names: "Domknięcie akustyki:220 x 150 cm:8812574", "Domknięcie akustyki:220 x 150 cm:8812805", "Domknięcie akustyki:220 x 150 cm:8812858" (+5 more) | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          127 x IFCBUILDINGELEMENTPROXY | object type "Podniesione" | names: "Domknięcie 38:Podniesione:8823751", "Domknięcie 38:Podniesione:8835215", "Domknięcie 38:Podniesione:8835225" (+124 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          210 x IFCBUILDINGELEMENTPROXY | object type "Płaskie" | names: "Domknięcie 38:Płaskie:8837909", "Domknięcie 38:Płaskie:8837957", "Domknięcie 38:Płaskie:8838002" (+207 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          2 x IFCDOOR | type IFCDOORSTYLE "2200 x 2375 ap" | object type "2200 x 2375 ap" | names: "Drzwi szklane 2skrz:2200 x 2375 ap:9120566", "Drzwi szklane 2skrz:2200 x 2375 ap:9120567" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "2150 x 2375 ap" | object type "2150 x 2375 ap" | names: "Drzwi szklane 2skrz:2150 x 2375 ap:9120568" | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "2200 x 2375 ap EZ" | object type "2200 x 2375 ap EZ" | names: "Drzwi szklane 2skrz:2200 x 2375 ap EZ:9120569" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCDOOR | type IFCDOORSTYLE "2155 x 2375 ap" | object type "2155 x 2375 ap" | names: "Drzwi szklane 2skrz:2155 x 2375 ap:9120572", "Drzwi szklane 2skrz:2155 x 2375 ap:9131651" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1900 x 2400 (120-70) ap" | object type "1900 x 2400 (120-70) ap" | names: "Drzwi szklane 2skrz:1900 x 2400 (120-70) ap:9121792" | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2400 Ra37" | object type "1100 x 2400 Ra37" | names: "Drzwi szklane 1skrz:1100 x 2400 Ra37:9125870" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "2200 x 2400 Ei-30 Ra32" | object type "2200 x 2400 Ei-30 Ra32" | names: "Drzwi szklane 2skrz:2200 x 2400 Ei-30 Ra32:9126746" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1180 x 2400 EI-30" | object type "1180 x 2400 EI-30" | names: "Drzwi szklane 1skrz:1180 x 2400 EI-30:9132033" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami 2 ROZW" | object type "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami 2 ROZW:13254339" | names: "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami 2 ROZW:9138912" | parts: 5 IFCMEMBER | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:wełna mineralna 5.5 cm" | object type "Basic Wall:wełna mineralna 5.5 cm:13091109" | names: "Basic Wall:wełna mineralna 5.5 cm:9145986", "Basic Wall:wełna mineralna 5.5 cm:9146288", "Basic Wall:wełna mineralna 5.5 cm:9146411" (+1 more) | material: layers "Basic Wall:wełna mineralna 5.5 cm" ("Welna Mineralna" 5.5) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:wełna mineralna 5 cm" | object type "Basic Wall:wełna mineralna 5 cm:4217669" | names: "Basic Wall:wełna mineralna 5 cm:9146177", "Basic Wall:wełna mineralna 5 cm:9148425" | material: layers "Basic Wall:wełna mineralna 5 cm" ("Welna Mineralna" 5.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "2400 X 2400" | object type "2400 X 2400" | names: "Drzwi szklane przesuwne:2400 X 2400:9182862" | material: materials ("SK- Szkło 2.5 cm", "Steel, Paint Finish, Ivory, Matte") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCSLAB | object type "Floor:S2 - Strop nad kanałem oddymiającym 20 cm" | FLOOR | names: "Floor:S2 - Strop nad kanałem oddymiającym 20 cm:9437475", "Floor:S2 - Strop nad kanałem oddymiającym 20 cm:9785828" | material: layers "Floor:S2 - Strop nad kanałem oddymiającym 20 cm" ("Beton Konstrukcja" 20.) | property sets: Other, Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties
          18 x IFCBUILDINGELEMENTPROXY | object type "Wnęka ROP śc szewron" | names: "Wnęka ROP śc szewron:Wnęka ROP śc szewron:9444577", "Wnęka ROP śc szewron:Wnęka ROP śc szewron:9444656", "Wnęka ROP śc szewron:Wnęka ROP śc szewron:9444812" (+15 more) | material: "Metal - Bronze" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Materials and Finishes
          25 x IFCBUILDINGELEMENTPROXY | object type "ROP model" | names: "ROP model:ROP model:9476578", "ROP model:ROP model:9477386", "ROP model:ROP model:9477488" (+22 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100" | object type "1100 x 2100" | names: "Drzwi drewniane 1skrz blokowe supraporta 1str:1100 x 2100:9761979" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2400 Ra37" | object type "1100 x 2400 Ra37" | names: "Drzwi szklane 1skrz:1100 x 2400 Ra37:9762805" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SK- Szkło 2.5 cm" | object type "Basic Wall:SK- Szkło 2.5 cm:9114278" | names: "Basic Wall:SK- Szkło 2.5 cm:9788902" | material: layers "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami" ("Glass" 2.5) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1200 x 2400 brąz" | object type "1200 x 2400 brąz" | names: "Drzwi stalowe 1skrz blokowe:1200 x 2400 brąz:9789241" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Metal - Bronze") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          4 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Surface Lamp PLEIAD G3 180 mm" | object type "MWP_M_Surface Lamp PLEIAD G3 180 mm" | names: "MWP_M_Surface Lamp round:MWP_M_Surface Lamp PLEIAD G3 180 mm:9789781", "MWP_M_Surface Lamp round:MWP_M_Surface Lamp PLEIAD G3 180 mm:9789783", "MWP_M_Surface Lamp round:MWP_M_Surface Lamp PLEIAD G3 180 mm:10078626" (+1 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCDOOR | type IFCDOORSTYLE "1200 x 2400" | object type "1200 x 2400" | names: "Drzwi indywidualne SWC Z:1200 x 2400:10012380" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1700 x 7300" | object type "1700 x 7300" | names: "Drzwi indywidualne SWC P:1700 x 7300:10014261" | material: "Copper bez podziału" | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          7 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK4 - Barierka podział 120 cm" | object type "Curtain Wall:SK4 - Barierka podział 120 cm:7571542" | names: "Curtain Wall:SK4 - Barierka podział 120 cm:10034355", "Curtain Wall:SK4 - Barierka podział 120 cm:10034678", "Curtain Wall:SK4 - Barierka podział 120 cm:10040998" (+4 more) | parts: 21 IFCPLATE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          8 x IFCBUILDINGELEMENTPROXY | object type "Kamera kopułkowa niżej" | names: "Kamera kopułkowa:Kamera kopułkowa niżej:10076427", "Kamera kopułkowa:Kamera kopułkowa niżej:12991410", "Kamera kopułkowa:Kamera kopułkowa niżej:13025295" (+5 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          20 x IFCBUILDINGELEMENTPROXY | object type "Kamera kopułkowa" | names: "Kamera kopułkowa:Kamera kopułkowa:10076464", "Kamera kopułkowa:Kamera kopułkowa:10076499", "Kamera kopułkowa:Kamera kopułkowa:10077040" (+17 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:krata nożycowa" | object type "Basic Wall:krata nożycowa:10396098" | names: "Basic Wall:krata nożycowa:10396258", "Basic Wall:krata nożycowa:10396565", "Basic Wall:krata nożycowa:10396727" (+7 more) | material: layers "Basic Wall:krata nożycowa" ("Default" 4.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1600 x 2100 (110-50) EI-30 KD1" | object type "1600 x 2100 (110-50) EI-30 KD1" | names: "Drzwi drewniane 2skrz blokowe supraporta 2str:1600 x 2100 (110-50) EI-30 KD1:10537732" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          25 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Bronze 0.8 mm" | object type "Basic Wall:Bronze 0.8 mm:11184046" | names: "Basic Wall:Bronze 0.8 mm:11192790", "Basic Wall:Bronze 0.8 mm:11192896", "Basic Wall:Bronze 0.8 mm:11193090" (+22 more) | material: layers "Basic Wall:Bronze 0.8 mm" ("Metal - Bronze" 0.8) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          18 x IFCBUILDINGELEMENTPROXY | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          4 x IFCSLAB | object type "Floor:S0 - Płyty Placu Gwardii 120 x 120 ryflowane" | FLOOR | names: "Floor:S0 - Płyty Placu Gwardii 120 x 120 ryflowane:11673769", "Floor:S0 - Płyty Placu Gwardii 120 x 120 ryflowane:11673862", "Floor:S0 - Płyty Placu Gwardii 120 x 120 ryflowane:11673931" (+1 more) | material: layers "Floor:S0 - Płyty Placu Gwardii 120 x 120 ryflowane" ("Płyty Placu Gwardii" 10.) | property sets: Other, Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties
          1 x IFCBUILDINGELEMENTPROXY | object type "Śrecnica 17 cm" | names: "Głośniki:Śrecnica 17 cm:11721378" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GKF EI-60 - 12,5cm" | object type "Basic Wall:GKF EI-60 - 12,5cm:12329376" | names: "Basic Wall:GKF EI-60 - 12,5cm:12330018", "Basic Wall:GKF EI-60 - 12,5cm:12330021" | material: layers "Basic Wall:GKF EI-60 - 12,5cm" ("Plasterboard" 1.25, "Plasterboard" 1.25, "Welna Mineralna" 7.5, "Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK 2 x 1.25" | object type "Basic Wall:GK 2 x 1.25:12360911" | names: "Basic Wall:GK 2 x 1.25:12360731", "Basic Wall:GK 2 x 1.25:12380103", "Basic Wall:GK 2 x 1.25:12380667" (+1 more) | material: layers "Basic Wall:GK 2 x 1.25" ("Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 6 cm" | object type "Basic Wall:SW1 - żelbet barwiony 6 cm:12378707" | names: "Basic Wall:SW1 - żelbet barwiony 6 cm:12378675", "Basic Wall:SW1 - żelbet barwiony 6 cm:12378853" | material: layers "Basic Wall:SW1 - żelbet barwiony 6 cm" ("Beton Barwiony Konstrukcja" 6.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          6 x IFCBUILDINGELEMENTPROXY | object type "PE model zielony" | names: "ROP model:PE model zielony:12792679", "ROP model:PE model zielony:12813711", "ROP model:PE model zielony:12884978" (+3 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "PE model zielony niższy" | names: "ROP model:PE model zielony niższy:12961869" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          2 x IFCBUILDINGELEMENTPROXY | object type "kamera on face" | names: "kamera on face:kamera on face:12976894", "kamera on face:kamera on face:12977225" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          6 x IFCBUILDINGELEMENTPROXY | object type "Type 1" | names: "gniazdko wxca:Type 1:13079026", "gniazdko wxca:Type 1:13079069", "gniazdko wxca:Type 1:13132472" (+3 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          8 x IFCBUILDINGELEMENTPROXY | object type "h 1.50" | names: "klawiatura KD:h 1.50:13160363", "klawiatura KD:h 1.50:13160856", "klawiatura KD:h 1.50:13160932" (+5 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          38 x IFCBUILDINGELEMENTPROXY | object type "h 1.72" | names: "czujnik TiW:h 1.72:13161953", "czujnik TiW:h 1.72:13162206", "czujnik TiW:h 1.72:13162327" (+35 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          56 x IFCBUILDINGELEMENTPROXY | object type "h 2.15" | names: "detektor dymu liniowy:h 2.15:13171267", "detektor dymu liniowy:h 2.15:13171574", "detektor dymu liniowy:h 2.15:13171611" (+53 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          3 x IFCSLAB | object type "Floor:ST - Krata wemna 3 cm" | FLOOR | names: "Floor:ST - Krata wemna 3 cm:13220519", "Floor:ST - Krata wemna 3 cm:13220519:2", "Floor:ST - Krata wemna 3 cm:13220519:3" | material: layers "Floor:ST - Krata wemna 3 cm" ("Krata Wema" 3.) | property sets: Other, Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties
          1 x IFCDOOR | type IFCDOORSTYLE "2142 x 2375 ap fasada rozwieralna" | object type "2142 x 2375 ap fasada rozwieralna" | names: "Drzwi szklane 2skrz:2142 x 2375 ap fasada rozwieralna:13254295" | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          14 x IFCBUILDINGELEMENTPROXY | object type "h 1.65" | names: "czujnik TiW:h 1.65:13303840", "czujnik TiW:h 1.65:13304005", "czujnik TiW:h 1.65:13304048" (+11 more) | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "listwa" | names: "listwa:listwa:13652223" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Electrical - Circuiting
          1 x IFCBUILDINGELEMENTPROXY | object type "Listwa 120 góra" | names: "Listwa 120 góra:Listwa 120 góra:13653203" | property sets: Other, Identity Data, Pset_BuildingElementProxyCommon, Constraints, Dimensions, Electrical - Circuiting
          1 x IFCRAILING | object type "Railing:Pełna policzkowa szpoczniki" | names: "Railing:Pełna policzkowa szpoczniki:7115179" | material: "Carbon Steel" | property sets: Top Rail, Other, Identity Data, Handrail 2, Handrail 1, Construction
      IFCBUILDINGSTOREY "101 rz.+333 Strop" | long name "101 rz.+333 Strop" | elevation 333.
        contains 110 elements
          54 x IFCBUILDINGELEMENTPROXY | object type "tryskacz korytarz" | names: "tryskacz:tryskacz korytarz:5321911", "tryskacz:tryskacz korytarz:5321921", "tryskacz:tryskacz korytarz:5321923" (+51 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 8 wc" | object type "LK 005.1 AG/ 8 wc" | names: "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 8 wc:5918627", "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 8 wc:5924228" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 9 wc" | object type "LK 005.1 AG/ 9 wc" | names: "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 9 wc:5919012", "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 9 wc:5924168" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle Wall:LK 005.1 AG/ 10wc:5924527" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          11 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "oświetlenie awaryjne D1W" | object type "oświetlenie awaryjne D1W" | names: "oświetlenie awaryjne:oświetlenie awaryjne D1W:7471958", "oświetlenie awaryjne:oświetlenie awaryjne D1W:7472056", "oświetlenie awaryjne:oświetlenie awaryjne D1W:7472228" (+8 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          26 x IFCBUILDINGELEMENTPROXY | object type "Śrecnica 17 cm" | names: "Głośniki:Śrecnica 17 cm:11687488", "Głośniki:Śrecnica 17 cm:11687525", "Głośniki:Śrecnica 17 cm:11691683" (+23 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          12 x IFCBUILDINGELEMENTPROXY | object type "wskaźnik zadziałania" | names: "wskaźnik zadziałania:wskaźnik zadziałania:11690540", "wskaźnik zadziałania:wskaźnik zadziałania:11690569", "wskaźnik zadziałania:wskaźnik zadziałania:11702511" (+9 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "oświetlenie awaryjne D3W" | object type "oświetlenie awaryjne D3W" | names: "oświetlenie awaryjne:oświetlenie awaryjne D3W:11691635" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          1 x IFCBUILDINGELEMENTPROXY | object type "Klamry" | names: "Drabinka:Klamry:13450897" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
      IFCBUILDINGSTOREY "101 rz. +345 Wyk." | long name "101 rz. +345 Wyk." | elevation 345.
        contains 66 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "Slab Edge:Nadciag 35x16cm" | names: "Slab Edge:Nadciag 35x16cm" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "tryskacz korytarz" | names: "tryskacz:tryskacz korytarz:5663121" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7639067" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          17 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7882740", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900725", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900726" (+14 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          7 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7888682", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900743", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900764" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900724", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900742", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900786" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900736", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900775" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900738" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          3 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900739", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900744", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900776" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900812", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8211945" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          7 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900814", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8211935", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:8211938" (+4 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900816" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:7927363" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          18 x IFCBUILDINGELEMENTPROXY | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "Śrecnica 17 cm" | names: "Głośniki:Śrecnica 17 cm:11721320" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
      IFCBUILDINGSTOREY "101 rz. +483 Strop" | long name "101 rz. +483 Strop" | elevation 483.000000000007
        contains 3 elements
          2 x IFCSLAB | object type "Floor:S4 - Strop między piętrami - 25 cm" | FLOOR | names: "Floor:S4 - Strop między piętrami - 25 cm:809945", "Floor:S4 - Strop między piętrami - 25 cm:1231766" | material: layers "Floor:S4 - Strop między piętrami - 25 cm" ("Beton Konstrukcja" 25.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 40 cm" | object type "Basic Wall:SW1 - żelbet barwiony 40 cm:221404" | names: "Basic Wall:SW1 - żelbet barwiony 40 cm:7324537" | material: layers "Basic Wall:SW1 - żelbet barwiony 40 cm" ("Beton Barwiony Konstrukcja" 40.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
      IFCBUILDINGSTOREY "101 rz. +495 Wyk." | long name "101 rz. +495 Wyk." | elevation 494.999999999984
        contains 145 elements
          1 x IFCWALL | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | object type "Basic Wall:SW2 - żelbet zwykły 20 cm:2377995" | names: "Basic Wall:SW2 - żelbet zwykły 20 cm:772490" | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 30 cm" | object type "Basic Wall:SW1 - żelbet barwiony 30 cm:536629" | names: "Basic Wall:SW1 - żelbet barwiony 30 cm:783297", "Basic Wall:SW1 - żelbet barwiony 30 cm:1209326", "Basic Wall:SW1 - żelbet barwiony 30 cm:1251323" (+2 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 30 cm" ("Beton Barwiony Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:wełna mineralna 20cm" | object type "Basic Wall:wełna mineralna 20cm:266360" | names: "Basic Wall:wełna mineralna 20cm:813422", "Basic Wall:wełna mineralna 20cm:813487", "Basic Wall:wełna mineralna 20cm:813593" (+5 more) | material: layers "Basic Wall:wełna mineralna 20cm" ("Insulation / Thermal Barriers - Rigid insulation" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | object type "Basic Wall:SW2 - żelbet zwykły 20 cm:2377995" | names: "Basic Wall:SW2 - żelbet zwykły 20 cm:817236", "Basic Wall:SW2 - żelbet zwykły 20 cm:817237", "Basic Wall:SW2 - żelbet zwykły 20 cm:1251329" (+1 more) | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 30 cm" | object type "Basic Wall:SW2 - żelbet zwykły 30 cm:4774648" | names: "Basic Wall:SW2 - żelbet zwykły 30 cm:1209615", "Basic Wall:SW2 - żelbet zwykły 30 cm:1210493", "Basic Wall:SW2 - żelbet zwykły 30 cm:1251328" (+2 more) | material: layers "Basic Wall:SW2 - żelbet zwykły 30 cm" ("Beton Konstrukcja" 30.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          18 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:203146" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:1209920", "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:1210051", "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm:1210306" (+15 more) | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" ("SILKA" 18.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm:203147" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm:1211264", "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm:1211440" | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm" ("SILKA" 8.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 SM" | object type "1100 x 2100 SM" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:1226310" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1200 x 2100" | object type "1200 x 2100" | names: "Drzwi drewniane 1skrz blokowe:1200 x 2100:1226311" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 SM" | object type "1100 x 2100 SM" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:1226312", "Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:1594433" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 blokada wc" | object type "1100 x 2100 blokada wc" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:1226313" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 blokada wc" | object type "1100 x 2100 blokada wc" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:1226320" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 20 cm" | object type "Basic Wall:SW1 - żelbet barwiony 20 cm:204370" | names: "Basic Wall:SW1 - żelbet barwiony 20 cm:1235493" | material: layers "Basic Wall:SW1 - żelbet barwiony 20 cm" ("Beton Barwiony Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCSLAB | object type "Floor:ST7 - Strop między piętrami - w.wykonczeniowe" | FLOOR | names: "Floor:ST7 - Strop między piętrami - w.wykonczeniowe:1597900", "Floor:ST7 - Strop między piętrami - w.wykonczeniowe:1597900:2", "Floor:ST7 - Strop między piętrami - w.wykonczeniowe:5615848" (+2 more) | material: layers "Floor:ST7 - Strop między piętrami - w.wykonczeniowe" ("Posadzka - wylewka betonowa" 7., "Styropian EPS - podłoga" 5.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym" | object type "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym:2431044" | names: "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym:1857951", "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym:1858075", "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym:4278319" (+2 more) | material: layers "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym" ("Folia kubełkowa / szczelina wentylacyjna" 5., "Beton Barwiony Okladzina" 5.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2" | object type "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2:249111" | names: "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2:1911451", "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2:2058820" | parts: 65 IFCMEMBER, 17 IFCWALLSTANDARDCASE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:ścianka instalacyjna 25 cm" | object type "Basic Wall:ścianka instalacyjna 25 cm:2392242" | names: "Basic Wall:ścianka instalacyjna 25 cm:2428408", "Basic Wall:ścianka instalacyjna 25 cm:2428663", "Basic Wall:ścianka instalacyjna 25 cm:2783838" | material: layers "Basic Wall:ścianka instalacyjna 25 cm" ("Default New Material Konstrukcja" 25.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:ścianka instalacyjna 13 cm" | object type "Basic Wall:ścianka instalacyjna 13 cm:2391863" | names: "Basic Wall:ścianka instalacyjna 13 cm:2428873" | material: layers "Basic Wall:ścianka instalacyjna 13 cm" ("Default New Material Konstrukcja" 13.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCSLAB | object type "Floor:ST9 - Strop między piętrami biura - w.wykonczeniowe" | FLOOR | names: "Floor:ST9 - Strop między piętrami biura - w.wykonczeniowe:2738617", "Floor:ST9 - Strop między piętrami biura - w.wykonczeniowe:2738617:2", "Floor:ST9 - Strop między piętrami biura - w.wykonczeniowe:2738617:3" (+2 more) | material: layers "Floor:ST9 - Strop między piętrami biura - w.wykonczeniowe" ("Posadzka_01" 2., "Posadzka - wylewka betonowa" 5., "Styropian EPS - podłoga" 5.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 blokada wc" | object type "1100 x 2100 blokada wc" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:2784990" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm" | object type "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm:4773790" | names: "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm:4274409", "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm:4277741" | material: layers "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm" ("Folia kubełkowa / szczelina wentylacyjna" 5., "Beton Barwiony Okladzina" 5.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm" | object type "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:1430568" | names: "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:4625465", "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:4625638", "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm:4625745" (+13 more) | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm" ("Beton Barwiony Konstrukcja" 15.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCSLAB | object type "Floor:D5 - Strop patio biura (warstwy wykończeniowe" | FLOOR | names: "Floor:D5 - Strop patio biura (warstwy wykończeniowe:4634330" | material: "Żwir drobnoziarnisty" | property sets: Other, Identity Data, Graphics, Construction, Analytical Properties, Pset_SlabCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "wpust 20 x 20 cm" | names: "wpust podłogowy:wpust 20 x 20 cm:4638387" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "DN 25" | names: "hydrant:DN 25:4648952" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          3 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza" | object type "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:4895782" | names: "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:4903245", "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:4903592", "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza:4904076" | parts: 21 IFCMEMBER, 4 IFCWALLSTANDARDCASE, 2 IFCPLATE | property sets: Pset_CurtainWallCommon, Constraints, Dimensions, Horizontal Grid, Identity Data, Other
          2 x IFCANNOTATION
          4 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 Ra32" | object type "1100 x 2100 Ra32" | names: "Drzwi drewniane 1skrz blokowe szklane SP:1100 x 2100 Ra32:5624212", "Drzwi drewniane 1skrz blokowe szklane SP:1100 x 2100 Ra32:5624250", "Drzwi drewniane 1skrz blokowe szklane SP:1100 x 2100 Ra32:5624267" (+1 more) | material: materials ("Door - Frame", "Door - Panel", "Glass") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCFLOWTERMINAL | object type "450 x 450mm" | names: "zlew 3d:450 x 450mm:7769102" | material: "Metal - Stainless Steel, Polished" | property sets: Other, Materials and Finishes, Identity Data, Dimensions, Pset_DistributionFlowElementCommon, Constraints
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900723", "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900785" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900741" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | object type "MWP_M_Ray Pendant" | names: "MWP_M_Surface Lamp round pendant:MWP_M_Ray Pendant:7900780" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | object type "Klamry" | names: "Drabinka:Klamry:7925940" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          1 x IFCDOOR | type IFCDOORSTYLE "0900 x 2100" | object type "0900 x 2100" | names: "Drzwi drewniane 1skrz blokowe:0900 x 2100:8053159" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1600 x 2400 (110-50) EI-30" | object type "1600 x 2400 (110-50) EI-30" | names: "Drzwi szklane 2skrz:1600 x 2400 (110-50) EI-30:9126849" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "2200 X 2400 zewn" | object type "2200 X 2400 zewn" | names: "Drzwi szklane 2skrz:2200 X 2400 zewn:9126955" | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          5 x IFCDOOR | type IFCDOORSTYLE "1140 x 2400 zewn" | object type "1140 x 2400 zewn" | names: "Drzwi szklane 1skrz:1140 x 2400 zewn:9129254", "Drzwi szklane 1skrz:1140 x 2400 zewn:9129339", "Drzwi szklane 1skrz:1140 x 2400 zewn:9129403" (+2 more) | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2400 Ra32" | object type "1100 x 2400 Ra32" | names: "Drzwi szklane 1skrz:1100 x 2400 Ra32:9132676" | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2400 Ra32" | object type "1100 x 2400 Ra32" | names: "Drzwi szklane 1skrz:1100 x 2400 Ra32:9132692" | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm" | object type "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:3295308" | names: "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:9768601", "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:9768602", "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm:9768603" (+3 more) | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm" ("SILKA" 12.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK 3cm" | object type "Basic Wall:GK 3cm:8093067" | names: "Basic Wall:GK 3cm:9768761", "Basic Wall:GK 3cm:10046242" | material: layers "Basic Wall:GK 3cm" ("Gypsum Wall Board" 3.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 SM" | object type "1100 x 2100 SM" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:9768762" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 SM" | object type "1100 x 2100 SM" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:9768765" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 blokada wc" | object type "1100 x 2100 blokada wc" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:9768768" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 blokada wc" | object type "1100 x 2100 blokada wc" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:9768769" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:ścianka instalacyjna 20 cm" | object type "Basic Wall:ścianka instalacyjna 20 cm:3783269" | names: "Basic Wall:ścianka instalacyjna 20 cm:9769963", "Basic Wall:ścianka instalacyjna 20 cm:9769964" | material: layers "Basic Wall:ścianka instalacyjna 20 cm" ("Default New Material Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1100 x 2100 SM" | object type "1100 x 2100 SM" | names: "Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:10045917" | material: materials ("Wood", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 10 cm" | object type "Basic Wall:SW1 (SZ3) - żelbet barwiony 10 cm:12379586" | names: "Basic Wall:SW1 (SZ3) - żelbet barwiony 10 cm:12314740" | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 10 cm" ("Beton Barwiony Konstrukcja" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GKF EI-60 - 12,5cm" | object type "Basic Wall:GKF EI-60 - 12,5cm:12329376" | names: "Basic Wall:GKF EI-60 - 12,5cm:12329461", "Basic Wall:GKF EI-60 - 12,5cm:12329977" | material: layers "Basic Wall:GKF EI-60 - 12,5cm" ("Plasterboard" 1.25, "Plasterboard" 1.25, "Welna Mineralna" 7.5, "Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK 2 x 1.25" | object type "Basic Wall:GK 2 x 1.25:12360911" | names: "Basic Wall:GK 2 x 1.25:12362504", "Basic Wall:GK 2 x 1.25:12380763", "Basic Wall:GK 2 x 1.25:12380808" | material: layers "Basic Wall:GK 2 x 1.25" ("Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:laminat 0,8 cm" | object type "Basic Wall:laminat 0,8 cm:12349527" | names: "Basic Wall:laminat 0,8 cm:12362715", "Basic Wall:laminat 0,8 cm:12362999", "Basic Wall:laminat 0,8 cm:12363000" (+1 more) | material: layers "Basic Wall:laminat 0,8 cm" ("Gypsum Wall Board" 0.8) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCBUILDINGELEMENTPROXY | object type "Type 1" | names: "głośnik PARTNER okragły wall base:Type 1:13479835" | property sets: Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints, Phasing
          1 x IFCRAILING | object type "Railing:Prostokątna wąska 15cm" | names: "Railing:Prostokątna wąska 15cm:12322832" | material: "Carbon Steel" | property sets: Top Rail, Other, Identity Data, Handrail 2, Handrail 1, Construction
      IFCBUILDINGSTOREY "101 rz. +690 Piętro Wyk." | long name "101 rz. +690 Piętro Wyk." | elevation 690.
        contains 16 elements
          16 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:GK 3cm" | object type "Basic Wall:GK 3cm:8093067" | names: "Basic Wall:GK 3cm:8093408", "Basic Wall:GK 3cm:8093449", "Basic Wall:GK 3cm:8093520" (+13 more) | material: layers "Basic Wall:GK 3cm" ("Gypsum Wall Board" 3.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
      IFCBUILDINGSTOREY "101 rz. +730" | long name "101 rz. +730" | elevation 730.000000000001
        contains 1668 elements
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF" | object type "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF:13616118" | names: "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF:1224459", "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF:1224460", "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF:1224615" (+1 more) | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF" ("Beton Barwiony Konstrukcja" 15.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          19 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SZ4 - Ocieplenie 18cm" | object type "Basic Wall:SZ4 - Ocieplenie 18cm:1471219" | names: "Basic Wall:SZ4 - Ocieplenie 18cm:1349730", "Basic Wall:SZ4 - Ocieplenie 18cm:1349770", "Basic Wall:SZ4 - Ocieplenie 18cm:1354912" (+16 more) | material: layers "Basic Wall:SZ4 - Ocieplenie 18cm" ("Insulation / Thermal Barriers - Rigid insulation" 18.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          337 x IFCBUILDINGELEMENTPROXY | object type "260 x 260" | names: "Moduł akustyczny Ekspozycja stała:260 x 260:4192629", "Moduł akustyczny Ekspozycja stała:260 x 260:4192813", "Moduł akustyczny Ekspozycja stała:260 x 260:4192868" (+334 more) | material: "Akustyka" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          1 x IFCBUILDINGELEMENTPROXY | object type "320 x 360" | names: "Moduł akustyczny Ekspozycja stała:320 x 360:4194914" | material: "Akustyka" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          120 x IFCBUILDINGELEMENTPROXY | object type "Moduł otwór duży T" | names: "Moduł betonowy Krzyż 360:Moduł otwór duży T:4197458", "Moduł betonowy Krzyż 360:Moduł otwór duży T:4197902", "Moduł betonowy Krzyż 360:Moduł otwór duży T:4197904" (+117 more) | material: "Beton Barwiony Konstrukcja" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          8 x IFCBUILDINGELEMENTPROXY | object type "Moduł otwór duży L1" | names: "Moduł betonowy Krzyż 360:Moduł otwór duży L1:4197590", "Moduł betonowy Krzyż 360:Moduł otwór duży L1:4198291", "Moduł betonowy Krzyż 360:Moduł otwór duży L1:4198358" (+5 more) | material: "Beton Barwiony Konstrukcja" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          8 x IFCBUILDINGELEMENTPROXY | object type "Moduł otwór duży L2" | names: "Moduł betonowy Krzyż 360:Moduł otwór duży L2:4197964", "Moduł betonowy Krzyż 360:Moduł otwór duży L2:4198284", "Moduł betonowy Krzyż 360:Moduł otwór duży L2:4198510" (+5 more) | material: "Beton Barwiony Konstrukcja" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          251 x IFCBUILDINGELEMENTPROXY | object type "Moduł otwór duży" | names: "Moduł betonowy Krzyż 360:Moduł otwór duży:4198022", "Moduł betonowy Krzyż 360:Moduł otwór duży:4198023", "Moduł betonowy Krzyż 360:Moduł otwór duży:4198026" (+248 more) | material: "Beton Barwiony Konstrukcja" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          12 x IFCBUILDINGELEMENTPROXY | object type "Moduł otwór duży S" | names: "Moduł betonowy Krzyż 360:Moduł otwór duży S:4198147", "Moduł betonowy Krzyż 360:Moduł otwór duży S:4198170", "Moduł betonowy Krzyż 360:Moduł otwór duży S:4198232" (+9 more) | material: "Beton Barwiony Konstrukcja" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          8 x IFCBUILDINGELEMENTPROXY | object type "Moduł SWO #1" | names: "Moduł betonowy Krzyż 360:Moduł SWO #1:4207123", "Moduł betonowy Krzyż 360:Moduł SWO #1:4207124", "Moduł betonowy Krzyż 360:Moduł SWO #1:4207126" (+5 more) | material: "Beton Barwiony Konstrukcja" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          568 x IFCBUILDINGELEMENTPROXY | object type "tryskacz korytarz" | names: "tryskacz:tryskacz korytarz:5301775", "tryskacz:tryskacz korytarz:5301778", "tryskacz:tryskacz korytarz:5301779" (+565 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          128 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "MWP_M_I-VALO ZETA 380mm" | object type "MWP_M_I-VALO ZETA 380mm" | names: "MWP_M_Recessed Exhibition ceiling:MWP_M_I-VALO ZETA 380mm:5719223", "MWP_M_Recessed Exhibition ceiling:MWP_M_I-VALO ZETA 380mm:5719475", "MWP_M_Recessed Exhibition ceiling:MWP_M_I-VALO ZETA 380mm:5719674" (+125 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          10 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "oświetlenie awaryjne D1W" | object type "oświetlenie awaryjne D1W" | names: "oświetlenie awaryjne:oświetlenie awaryjne D1W:6655222", "oświetlenie awaryjne:oświetlenie awaryjne D1W:6655366", "oświetlenie awaryjne:oświetlenie awaryjne D1W:6655642" (+7 more) | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Identity Data, Other
          4 x IFCBUILDINGELEMENTPROXY | object type "0" | names: "Moduł akustyczny opaska:0:7507322", "Moduł akustyczny opaska:0:7507790", "Moduł akustyczny opaska:0:7507864" (+1 more) | material: "Akustyka" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Materials and Finishes
          150 x IFCBUILDINGELEMENTPROXY | object type "Śrecnica 17 cm" | names: "Głośniki:Śrecnica 17 cm:8451055", "Głośniki:Śrecnica 17 cm:8451820", "Głośniki:Śrecnica 17 cm:8451821" (+147 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          2 x IFCBUILDINGELEMENTPROXY | object type "Moduł SWO T2" | names: "Moduł betonowy Krzyż 360:Moduł SWO T2:8563373", "Moduł betonowy Krzyż 360:Moduł SWO T2:8563609" | material: "Beton Barwiony Konstrukcja" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Materials and Finishes
          2 x IFCBUILDINGELEMENTPROXY | object type "Moduł SWO T1" | names: "Moduł betonowy Krzyż 360:Moduł SWO T1:8563476", "Moduł betonowy Krzyż 360:Moduł SWO T1:8563580" | material: "Beton Barwiony Konstrukcja" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Materials and Finishes
          2 x IFCBUILDINGELEMENTPROXY | object type "260 x 260 cm" | names: "Domknięcie akustyki:260 x 260 cm:8799187", "Domknięcie akustyki:260 x 260 cm:8799189" | property sets: Visibility, Other, Identity Data, Dimensions, Pset_BuildingElementProxyCommon, Constraints
          2 x IFCFLOWTERMINAL | type IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | object type "LK 005.1 AG/ 10wc" | names: "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:10410750", "MWP_M_Downlight - Recessed rectangle K1:LK 005.1 AG/ 10wc:10410751" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, Electrical - Lighting, Electrical - Loads, Identity Data
          31 x IFCBUILDINGELEMENTPROXY | object type "symbol 10" | names: "głowica systemu zasysającego:symbol 10:10971313", "głowica systemu zasysającego:symbol 10:10972298", "głowica systemu zasysającego:symbol 10:10972340" (+28 more) | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
          1 x IFCBUILDINGELEMENTPROXY | object type "Wywiewka" | names: "Wywiewka:Wywiewka:11424494" | property sets: Other, Identity Data, Dimensions, Constraints, Pset_BuildingElementProxyCommon, Phasing
      IFCBUILDINGSTOREY "102 rz. +775 Mostek Techn." | long name "102 rz. +775 Mostek Techn." | elevation 775.000000000007
        contains 44 elements
          2 x IFCSLAB | object type "Floor:ST8 - Strop mosek techniczny, żelbet 25 cm" | FLOOR | names: "Floor:ST8 - Strop mosek techniczny, żelbet 25 cm:764044", "Floor:ST8 - Strop mosek techniczny, żelbet 25 cm:7900572" | material: layers "Floor:ST8 - Strop mosek techniczny, żelbet 25 cm" ("Beton Konstrukcja" 25.) | property sets: Pset_SlabCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | object type "Basic Wall:SW2 - żelbet zwykły 20 cm:2377995" | names: "Basic Wall:SW2 - żelbet zwykły 20 cm:4602723", "Basic Wall:SW2 - żelbet zwykły 20 cm:4603696", "Basic Wall:SW2 - żelbet zwykły 20 cm:4604027" (+3 more) | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 40 cm" | object type "Basic Wall:SW1 - żelbet barwiony 40 cm:221404" | names: "Basic Wall:SW1 - żelbet barwiony 40 cm:4772257", "Basic Wall:SW1 - żelbet barwiony 40 cm:4772258", "Basic Wall:SW1 - żelbet barwiony 40 cm:4772259" (+5 more) | material: layers "Basic Wall:SW1 - żelbet barwiony 40 cm" ("Beton Barwiony Konstrukcja" 40.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          1 x IFCDOOR | type IFCDOORSTYLE "1000 x 200 Ra37" | object type "1000 x 200 Ra37" | names: "Drzwi stalowe 1skrz blokowe:1000 x 200 Ra37:5941210" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          3 x IFCDOOR | type IFCDOORSTYLE "1000 x 200 Ra37" | object type "1000 x 200 Ra37" | names: "Drzwi stalowe 1skrz blokowe:1000 x 200 Ra37:5941281", "Drzwi stalowe 1skrz blokowe:1000 x 200 Ra37:5941328", "Drzwi stalowe 1skrz blokowe:1000 x 200 Ra37:5941423" | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Pset_DoorCommon, Constraints, Dimensions, Identity Data, Materials and Finishes, Other
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:SZ4 - Ocieplenie 18cm" | object type "Basic Wall:SZ4 - Ocieplenie 18cm:1471219" | names: "Basic Wall:SZ4 - Ocieplenie 18cm:7705254", "Basic Wall:SZ4 - Ocieplenie 18cm:7710491", "Basic Wall:SZ4 - Ocieplenie 18cm:7710563" (+5 more) | material: layers "Basic Wall:SZ4 - Ocieplenie 18cm" ("Insulation / Thermal Barriers - Rigid insulation" 18.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural
          5 x IFCSLAB | object type "Floor:ST - Krata wemna 3 cm" | FLOOR | names: "Floor:ST - Krata wemna 3 cm:8814989", "Floor:ST - Krata wemna 3 cm:8814989:2", "Floor:ST - Krata wemna 3 cm:8814989:3" (+2 more) | material: layers "Floor:ST - Krata wemna 3 cm" ("Krata Wema" 3.) | property sets: Other, Materials and Finishes, Identity Data, Graphics, Construction, Analytical Properties
          11 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:wełna minerlana 10 cm" | object type "Basic Wall:wełna minerlana 10 cm:10786936" | names: "Basic Wall:wełna minerlana 10 cm:10787037", "Basic Wall:wełna minerlana 10 cm:10787094", "Basic Wall:wełna minerlana 10 cm:10787334" (+8 more) | material: layers "Basic Wall:wełna minerlana 10 cm" ("Insulation / Thermal Barriers - Rigid insulation" 10.) | property sets: Constraints, Dimensions, Identity Data, Other, Phasing, Structural

Types
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 30 cm" | STANDARD | 20 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 30 cm" ("Beton Barwiony Konstrukcja" 30.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 20 cm" | STANDARD | 23 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 20 cm" ("Beton Barwiony Konstrukcja" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 50 cm" | STANDARD | 1 occurrence | material: layers "Basic Wall:SW1 - żelbet barwiony 50 cm" ("Beton Barwiony Konstrukcja" 50.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 30 cm" | STANDARD | 10 occurrences | material: layers "Basic Wall:SW2 - żelbet zwykły 30 cm" ("Beton Konstrukcja" 30.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 20 cm" | STANDARD | 23 occurrences | material: layers "Basic Wall:SW2 - żelbet zwykły 20 cm" ("Beton Konstrukcja" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 25 cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 25 cm" ("Beton Barwiony Konstrukcja" 25.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 40 cm" | STANDARD | 38 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 40 cm" ("Beton Barwiony Konstrukcja" 40.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:GKF EI-60 - 12,5cm" | STANDARD | 6 occurrences | material: layers "Basic Wall:GKF EI-60 - 12,5cm" ("Plasterboard" 1.25, "Plasterboard" 1.25, "Welna Mineralna" 7.5, "Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:laminat 0,8 cm" | STANDARD | 19 occurrences | material: layers "Basic Wall:laminat 0,8 cm" ("Gypsum Wall Board" 0.8) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:GK 2 x 1.25" | STANDARD | 10 occurrences | material: layers "Basic Wall:GK 2 x 1.25" ("Plasterboard" 1.25, "Plasterboard" 1.25) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:styrodur 20 cm" | STANDARD | 1 occurrence | material: layers "Basic Wall:styrodur 20 cm" ("Polistyren Ekstrudowany - izolacja termiczna - do znacznych obciążeń" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 3 occurrences | property sets: Constraints, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 15 cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:SW2 - żelbet zwykły 15 cm" ("Beton Konstrukcja" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:GK-C50-2x12,5cm" | STANDARD | 1 occurrence | material: layers "Basic Wall:GK-C50-2x12,5cm" ("Plasterboard" 1.25, "Plasterboard" 1.25, "Welna Mineralna" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm" | STANDARD | 24 occurrences | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm" ("Beton Barwiony Konstrukcja" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej" | STANDARD | 7 occurrences | material: layers "Basic Wall:SZ1 - obudowa zewn. przy 40 cm barwionej" ("Beton Barwiony Konstrukcja" 20., "Folia kubełkowa / szczelina wentylacyjna" 1., "Insulation / Thermal Barriers - Rigid insulation" 19.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:SZ5 - obudowa zewnętrzna wnęk" | STANDARD | 10 occurrences | material: layers "Basic Wall:SZ5 - obudowa zewnętrzna wnęk" ("Beton Barwiony Konstrukcja" 15., "Insulation / Thermal Barriers - Rigid insulation" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1100 x 2100 KT" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Door - Frame", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100 KT:677092, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1200 x 2100" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe supraporta 2str:1200 x 2100:677229, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCDOORSTYLE "1200 x 2400 brąz" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Metal - Bronze") | property sets: Drzwi stalowe 1skrz blokowe:1200 x 2400 brąz:677510, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami" | 6 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCCURTAINWALLTYPE "Curtain Wall:SK4 - Sciana kurtynowa wnętrza pusta" | 2 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 70cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 70cm" ("Beton Barwiony Konstrukcja" 70.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" | STANDARD | 33 occurrences | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 18 cm" ("SILKA" 18.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100:1462375, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCWALLTYPE "Basic Wall:SW3 - bloczki betonowe 18 cm" | STANDARD | 5 occurrences | material: layers "Basic Wall:SW3 - bloczki betonowe 18 cm" ("Beton bloczki" 18.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Door - Frame", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:SW2 - żelbet zwykły 40 cm" | STANDARD | 1 occurrence | material: layers "Basic Wall:SW2 - żelbet zwykły 40 cm" ("Beton Konstrukcja" 40.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:ścianka instalacyjna 13 cm" | STANDARD | 8 occurrences | material: layers "Basic Wall:ścianka instalacyjna 13 cm" ("Default New Material Konstrukcja" 13.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:ścianka instalacyjna 25 cm" | STANDARD | 8 occurrences | material: layers "Basic Wall:ścianka instalacyjna 25 cm" ("Default New Material Konstrukcja" 25.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCOLUMNTYPE "40 x 40 cm" | element type "40 x 40 cm" | COLUMN | 6 occurrences | property sets: Dimensions, Graphics, Identity Data, Other
  IFCDOORSTYLE "1200 x 2400 beton EI-30" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Drzwi stalowe 1skrz blokowe:1200 x 2400 beton EI-30:2620844, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2" | 4 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCDOORSTYLE "1100 x 2100 Ra32 KD2" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra32 KD2:2849913, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCDOORSTYLE "1100 x 2100 Ra27" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra27:3273618, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCDOORSTYLE "1100 x 2100 blokada wc" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm" | STANDARD | 4 occurrences | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 8 cm" ("SILKA" 8.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100" | SINGLE_SWING_LEFT | 2 occurrences | material: materials ("Wood", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe supraporta 1str:1100 x 2100:3276145, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCDOORSTYLE "1100 x 2100 Ra32 KD2" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:SW8 - okładzina SWC" | STANDARD | 4 occurrences | material: layers "Basic Wall:SW8 - okładzina SWC" ("Copper z podziałem" 5., "Welna Mineralna Akustyka" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1900 x 2400 (podział 110 80) ap beton poprawione" | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Beton Barwiony Konstrukcja") | property sets: Drzwi stalowe 2skrz niesym blokowe:1900 x 2400 (podział 110 80) ap beton poprawione:4071345, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:wełna minerlana 12 cm" | STANDARD | 4 occurrences | material: layers "Basic Wall:wełna minerlana 12 cm" ("Insulation / Thermal Barriers - Rigid insulation" 12.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCCURTAINWALLTYPE "Curtain Wall:SK5_Podkonstrukcja" | 1 occurrence | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.)" | STANDARD | 18 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 3 cm (6 cm) (pł. demont.)" ("Beton Barwiony Okladzina" 3.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCCURTAINWALLTYPE "Curtain Wall:SK6 - Sciana kurtynowa profilowa wnętrza" | 5 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm" | STANDARD | 11 occurrences | material: layers "Basic Wall:SW4 - bloczki silikatowe tynkowane 12 cm" ("SILKA" 12.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 183 mm" | 20 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 183 mm" | 3 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "TRIL 20.1030.35 116mm" | 20 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 183 mm" | 19 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "Pleiad Comfort G3 110 mm" | 17 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "Pozzo Delta 550mm" | 12 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "CSALP TRI 60.1041.15 143mm" | 16 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "MWP_M_Surface Lamp PLEIAD G3 180 mm" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:laminat 3cm" | STANDARD | 7 occurrences | material: layers "Basic Wall:laminat 3cm" ("Gypsum Wall Board" 3.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1900 x 2400 mm (podział 110 80) EI-30 ap beton poprawione" | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Beton Barwiony Okladzina") | property sets: Drzwi stalowe 2skrz niesym blokowe:1900 x 2400 mm (podział 110 80) EI-30 ap beton poprawione:7117541, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:SW6 - okł. miedziana SWC 5 cm" | STANDARD | 8 occurrences | material: layers "Basic Wall:SW6 - okł. miedziana SWC 5 cm" ("Copper bez podziału" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy" | STANDARD | 4 occurrences | material: layers "Basic Wall:SW7 - okł. miedziana SWC 5 cm + inne warstwy" ("Copper bez podziału" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:SW3 - bloczki betonowe 20 cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:SW3 - bloczki betonowe 20 cm" ("Beton bloczki" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1175 x 2400 + 4800 sp" | SINGLE_SWING_LEFT | 1 occurrence | material: "Copper bez podziału" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7133277
  IFCDOORSTYLE "1175 x 2400 + 4800 sp" | SINGLE_SWING_LEFT | 1 occurrence | material: "Copper bez podziału" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7137746
  IFCDOORSTYLE "1175 x 2400 + 4800 sp" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Copper bez podziału" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7137829
  IFCDOORSTYLE "1175 x 2400 + 4800 sp" | SINGLE_SWING_RIGHT | 1 occurrence | material: "Copper bez podziału" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7138385
  IFCDOORSTYLE "3275 x 7150 + 50 sp" | SINGLE_SWING_LEFT | 1 occurrence | material: "Copper bez podziału" | property sets: Drzwi indywidualne SWC blokowe:3275 x 7150 + 50 sp:7138557, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 10 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Surface Lamp Kaptur LITE 600mm" | 6 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "szynoprzewod" | 4 occurrences | property sets: Identity Data, Other
  IFCLIGHTFIXTURETYPE "szynoprzewod" | 1 occurrence | property sets: Identity Data, Other
  IFCLIGHTFIXTURETYPE "szynoprzewod" | 1 occurrence | property sets: Identity Data, Other
  IFCLIGHTFIXTURETYPE "TRIL 20.1030.35 116mm" | 6 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 6 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 11 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "1100 x 2400 (beton)" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Beton Barwiony Okladzina") | property sets: Drzwi stalowe 1skrz blokowe:1100 x 2400 (beton):7898971, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "TRIL 20.1030.25 116mm" | 279 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:GK 3cm" | STANDARD | 27 occurrences | material: layers "Basic Wall:GK 3cm" ("Gypsum Wall Board" 3.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCLIGHTFIXTURETYPE "szynoprzewod" | 1 occurrence | property sets: Identity Data, Other
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 3 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCWALLTYPE "Basic Wall:GK wełna GK" | STANDARD | 1 occurrence | material: layers "Basic Wall:GK wełna GK" ("Gypsum Wall Board" 1.25, "Insulation / Thermal Barriers - Rigid insulation" 7., "Gypsum Wall Board" 1.25) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 9 wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 9 wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" | 46 occurrences | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCLIGHTFIXTURETYPE "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" | 1 occurrence | property sets: Dimensions, Electrical, Electrical - Loads, Identity Data, Other, Photometrics
  IFCDOORSTYLE "1100 x 2100" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Drzwi stalowe 1skrz blokowe:1100 x 2100:8563773, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCWALLTYPE "Basic Wall:wełna minerlana 15 cm" | STANDARD | 11 occurrences | material: layers "Basic Wall:wełna minerlana 15 cm" ("Insulation / Thermal Barriers - Rigid insulation" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "2200 x 2375 ap" | 2 occurrences | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2200 x 2375 ap:9120566, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "2150 x 2375 ap" | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2150 x 2375 ap:9120568, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "2200 x 2375 ap EZ" | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2200 x 2375 ap EZ:9120569, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "2155 x 2375 ap" | 2 occurrences | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2155 x 2375 ap:9120572, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1900 x 2400 (120-70) ap" | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2400 Ra37" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 1skrz:1100 x 2400 Ra37:9125870, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "2200 x 2400 Ei-30 Ra32" | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2200 x 2400 Ei-30 Ra32:9126746, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1180 x 2400 EI-30" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 1skrz:1180 x 2400 EI-30:9132033, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCCURTAINWALLTYPE "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami 2 ROZW" | 1 occurrence | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:wełna mineralna 5.5 cm" | STANDARD | 4 occurrences | material: layers "Basic Wall:wełna mineralna 5.5 cm" ("Welna Mineralna" 5.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:wełna mineralna 5 cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:wełna mineralna 5 cm" ("Welna Mineralna" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "2400 X 2400" | 1 occurrence | material: materials ("SK- Szkło 2.5 cm", "Steel, Paint Finish, Ivory, Matte") | property sets: Drzwi szklane przesuwne:2400 X 2400:9182862, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1100 x 2100" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1100 x 2400 Ra37" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SK- Szkło 2.5 cm" | STANDARD | 1 occurrence | material: layers "Curtain Wall:SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami" ("Glass" 2.5) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1200 x 2400 brąz" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Metal - Bronze") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCLIGHTFIXTURETYPE "MWP_M_Surface Lamp PLEIAD G3 180 mm" | 4 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "1200 x 2400" | SINGLE_SWING_LEFT | 1 occurrence | material: "Copper bez podziału" | property sets: Drzwi indywidualne SWC Z:1200 x 2400:10012380, Analytical Properties, Construction, Dimensions, Identity Data, Other
  IFCDOORSTYLE "1700 x 7300" | 1 occurrence | material: "Copper bez podziału" | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Other, Drzwi indywidualne SWC P:1700 x 7300:10014261
  IFCCURTAINWALLTYPE "Curtain Wall:SK4 - Barierka podział 120 cm" | 7 occurrences | property sets: Construction, Horizontal Grid, Horizontal Mullions, Identity Data, Other, Vertical Grid
  IFCWALLTYPE "Basic Wall:krata nożycowa" | STANDARD | 10 occurrences | material: layers "Basic Wall:krata nożycowa" ("Default" 4.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1600 x 2100 (110-50) EI-30 KD1" | DOUBLE_DOOR_SINGLE_SWING | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Drzwi drewniane 2skrz blokowe supraporta 2str:1600 x 2100 (110-50) EI-30 KD1:10537732, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:Bronze 0.8 mm" | STANDARD | 25 occurrences | material: layers "Basic Wall:Bronze 0.8 mm" ("Metal - Bronze" 0.8) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCWALLTYPE "Basic Wall:SW1 - żelbet barwiony 6 cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:SW1 - żelbet barwiony 6 cm" ("Beton Barwiony Konstrukcja" 6.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "2142 x 2375 ap fasada rozwieralna" | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2142 x 2375 ap fasada rozwieralna:13254295, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 8 wc" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 9 wc" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "oświetlenie awaryjne D1W" | 21 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "oświetlenie awaryjne D3W" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 17 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 7 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 3 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 3 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 7 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "LK 005.1 AG/ 10wc" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other
  IFCWALLTYPE "Basic Wall:wełna mineralna 20cm" | STANDARD | 8 occurrences | material: layers "Basic Wall:wełna mineralna 20cm" ("Insulation / Thermal Barriers - Rigid insulation" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1100 x 2100 SM" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:1226310, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1200 x 2100" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe:1200 x 2100:1226311, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCDOORSTYLE "1100 x 2100 SM" | SINGLE_SWING_RIGHT | 2 occurrences | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100 blokada wc" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1100 x 2100 blokada wc" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym" | STANDARD | 5 occurrences | material: layers "Basic Wall:SZ6 - pł. bet. 5cm przy żelbecie barwionym" ("Folia kubełkowa / szczelina wentylacyjna" 5., "Beton Barwiony Okladzina" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1100 x 2100 blokada wc" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:SZ7 - pł. bet. 3cm + 20cm żelbet + pł. bet. 3cm" ("Folia kubełkowa / szczelina wentylacyjna" 5., "Beton Barwiony Okladzina" 5.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCDOORSTYLE "1100 x 2100 Ra32" | SINGLE_SWING_RIGHT | 4 occurrences | material: materials ("Door - Frame", "Door - Panel", "Glass") | property sets: Drzwi drewniane 1skrz blokowe szklane SP:1100 x 2100 Ra32:5624212, Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 2 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCLIGHTFIXTURETYPE "MWP_M_Ray Pendant" | 1 occurrence | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "0900 x 2100" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Drzwi drewniane 1skrz blokowe:0900 x 2100:8053159, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1600 x 2400 (110-50) EI-30" | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:1600 x 2400 (110-50) EI-30:9126849, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "2200 X 2400 zewn" | 1 occurrence | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 2skrz:2200 X 2400 zewn:9126955, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1140 x 2400 zewn" | SINGLE_SWING_LEFT | 5 occurrences | material: materials ("Metal - Aluminum", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 1skrz:1140 x 2400 zewn:9129254, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1100 x 2400 Ra32" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Drzwi szklane 1skrz:1100 x 2400 Ra32:9132676, Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1100 x 2400 Ra32" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "SK- Szkło 2.5 cm") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100 SM" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100 SM" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100 blokada wc" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCDOORSTYLE "1100 x 2100 blokada wc" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Green Building Properties, Identity Data, Materials and Finishes
  IFCWALLTYPE "Basic Wall:ścianka instalacyjna 20 cm" | STANDARD | 2 occurrences | material: layers "Basic Wall:ścianka instalacyjna 20 cm" ("Default New Material Konstrukcja" 20.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1100 x 2100 SM" | SINGLE_SWING_RIGHT | 1 occurrence | material: materials ("Wood", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 10 cm" | STANDARD | 1 occurrence | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 10 cm" ("Beton Barwiony Konstrukcja" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF" | STANDARD | 4 occurrences | material: layers "Basic Wall:SW1 (SZ3) - żelbet barwiony 15 cm PREF" ("Beton Barwiony Konstrukcja" 15.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:SZ4 - Ocieplenie 18cm" | STANDARD | 27 occurrences | material: layers "Basic Wall:SZ4 - Ocieplenie 18cm" ("Insulation / Thermal Barriers - Rigid insulation" 18.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCLIGHTFIXTURETYPE "MWP_M_I-VALO ZETA 380mm" | 128 occurrences | property sets: Constraints, Dimensions, Identity Data, Other, Text
  IFCDOORSTYLE "1000 x 200 Ra37" | SINGLE_SWING_LEFT | 1 occurrence | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCDOORSTYLE "1000 x 200 Ra37" | SINGLE_SWING_RIGHT | 3 occurrences | material: materials ("Steel, Paint Finish, Ivory, Matte", "Door - Panel") | property sets: Analytical Properties, Construction, Dimensions, Identity Data, Materials and Finishes, Other
  IFCWALLTYPE "Basic Wall:wełna minerlana 10 cm" | STANDARD | 11 occurrences | material: layers "Basic Wall:wełna minerlana 10 cm" ("Insulation / Thermal Barriers - Rigid insulation" 10.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other

Property sets
  Text | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Rewizja wewn. = "02.2.05" (IFCTEXT)
  Text | properties | on 25 type objects
    Rodzaj = "natynkowe" (IFCTEXT)
  Text | properties | on 15 type objects
    Rodzaj = "wpuszczane" (IFCTEXT)
  Text | properties | on 2 type objects
    nazwa = "AW" (IFCTEXT)
  Other | properties | on 1070 objects (1070 IFCOPENINGELEMENT)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Ściągi" (IFCTEXT)
  Other | properties | on 627 objects (627 IFCOPENINGELEMENT)
    Category = "Generic Models" (IFCLABEL)
    Family = "Ściągi: R120 H 720" (IFCLABEL)
    Family and Type = "Ściągi: R120 H 720" (IFCLABEL)
    Host Id = "Basic Wall: SW1 - żelbet barwiony 40 cm" (IFCLABEL)
    Type = "Ściągi: R120 H 720" (IFCLABEL)
    Type Id = "Ściągi: R120 H 720" (IFCLABEL)
  Other | properties | on 623 objects (623 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "tryskacz" (IFCTEXT)
  Other | properties | on 494 objects (494 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "tryskacz: tryskacz korytarz" (IFCLABEL)
    Family and Type = "tryskacz: tryskacz korytarz" (IFCLABEL)
    Schedule Level = "Level: 100 rz. 0.00 - Parter" (IFCLABEL)
    Type = "tryskacz: tryskacz korytarz" (IFCLABEL)
    Type Id = "tryskacz: tryskacz korytarz" (IFCLABEL)
  Other | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Domknięcie akustyki" (IFCTEXT)
    Ilość = 5. (IFCREAL)
    Ilość trapezów = 5 (IFCINTEGER)
  Other | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Moduł akustyczny Ekspozycja stała: 260 x 260" (IFCLABEL)
    Family and Type = "Moduł akustyczny Ekspozycja stała: 260 x 260" (IFCLABEL)
    Schedule Level = "Level: 099 rz. -374" (IFCLABEL)
    Type = "Moduł akustyczny Ekspozycja stała: 260 x 260" (IFCLABEL)
    Type Id = "Moduł akustyczny Ekspozycja stała: 260 x 260" (IFCLABEL)
  Other | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Moduł akustyczny Ekspozycja stała" (IFCTEXT)
    dziurawy = FALSE (IFCBOOLEAN)
    pełny = TRUE (IFCBOOLEAN)
  Other | properties | on 279 objects (279 IFCFLOWTERMINAL)
    Category = "Lighting Fixtures" (IFCLABEL)
    Family = "MWP_M_Downlight - Recessed Can: TRIL 20.1030.25 116mm" (IFCLABEL)
    Family and Type = "MWP_M_Downlight - Recessed Can: TRIL 20.1030.25 116mm" (IFCLABEL)
    Host Id = "Compound Ceiling: SAK 1" (IFCLABEL)
    Type = "MWP_M_Downlight - Recessed Can: TRIL 20.1030.25 116mm" (IFCLABEL)
    Type Id = "MWP_M_Downlight - Recessed Can: TRIL 20.1030.25 116mm" (IFCLABEL)
    widoczność = FALSE (IFCBOOLEAN)
  Other: 441 more contents on 6851 objects not shown
  Identity Data | properties | on 1216 objects (1216 IFCOPENINGELEMENT)
    Edited by = "" (IFCTEXT)
    Workset = "011_ŚCIĄGI" (IFCIDENTIFIER)
  Identity Data | properties | on 1170 objects (1147 IFCBUILDINGELEMENTPROXY, 8 IFCFLOWTERMINAL, 5 IFCOPENINGELEMENT, 4 IFCGROUP)
    Edited by = "" (IFCTEXT)
    Workset = "080_INSTALACJE" (IFCIDENTIFIER)
  Identity Data | properties | on 1070 objects (1070 IFCOPENINGELEMENT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Edited by = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "R120 H 720" (IFCTEXT)
    Workset = "Family : Generic Models : Ściągi" (IFCIDENTIFIER)
  Identity Data | properties | on 1012 objects (758 IFCBUILDINGELEMENTPROXY, 81 IFCOPENINGELEMENT, 65 IFCWALLSTANDARDCASE, 35 IFCSLAB)
    Edited by = "" (IFCTEXT)
    Workset = "060_WYKOŃCZENIA" (IFCIDENTIFIER)
  Identity Data | properties | on 836 objects (831 IFCBUILDINGELEMENTPROXY, 5 IFCGROUP)
    Edited by = "" (IFCTEXT)
    Workset = "060_WYKOŃCZENIA - konstrukcje stalowe" (IFCIDENTIFIER)
  Identity Data | properties | on 623 objects (623 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Edited by = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Mark = "tryskacz" (IFCTEXT)
    Type Name = "tryskacz korytarz" (IFCTEXT)
    Workset = "Family : Generic Models : tryskacz" (IFCIDENTIFIER)
  Identity Data | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Edited by = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "260 x 260 cm" (IFCTEXT)
    Workset = "Family : Generic Models : Domknięcie akustyki" (IFCIDENTIFIER)
  Identity Data | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Edited by = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "260 x 260" (IFCTEXT)
    Workset = "Family : Generic Models : Moduł akustyczny Ekspozycja stała" (IFCIDENTIFIER)
  Identity Data: 1053 more contents on 4354 objects not shown
  Dimensions | properties | on 1070 objects (1070 IFCOPENINGELEMENT)
    Offset od posadzki = 51. (IFCLENGTHMEASURE) [CENTI METRE]
    Rozstaw = 120. (IFCLENGTHMEASURE) [CENTI METRE]
    Symbol = 4.4 (IFCLENGTHMEASURE) [CENTI METRE]
    Średnica ściągu = 2.2 (IFCLENGTHMEASURE) [CENTI METRE]
  Dimensions | properties | on 623 objects (623 IFCBUILDINGELEMENTPROXY)
    Offset = 15. (IFCLENGTHMEASURE) [CENTI METRE]
    Wysokość = 20. (IFCLENGTHMEASURE) [CENTI METRE]
    głębokość = 2. (IFCLENGTHMEASURE) [CENTI METRE]
    Średnica = 4. (IFCLENGTHMEASURE) [CENTI METRE]
  Dimensions | properties | on 623 objects (623 IFCBUILDINGELEMENTPROXY)
    Area = 0.0138228396596068 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000251319231710384 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 399 objects (399 IFCBUILDINGELEMENTPROXY)
    Boczny otwór 2 = 12. (IFCLENGTHMEASURE) [CENTI METRE]
    Boczny otwór = 12. (IFCLENGTHMEASURE) [CENTI METRE]
    Grubość_Modułu = 10. (IFCLENGTHMEASURE) [CENTI METRE]
    Krawędziowy otwór = 15. (IFCLENGTHMEASURE) [CENTI METRE]
    Rozpiętość modułu = 360. (IFCLENGTHMEASURE) [CENTI METRE]
    Szerokość ramienia = 100. (IFCLENGTHMEASURE) [CENTI METRE]
    moduł = 120. (IFCLENGTHMEASURE) [CENTI METRE]
    Średnica słupa = 48. (IFCLENGTHMEASURE) [CENTI METRE]
    Środkowy otwór = 40. (IFCLENGTHMEASURE) [CENTI METRE]
  Dimensions | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Dł. kątownika = 20. (IFCLENGTHMEASURE) [CENTI METRE]
    Offset = 76. (IFCLENGTHMEASURE) [CENTI METRE]
    Profil = 5. (IFCLENGTHMEASURE) [CENTI METRE]
    Rozpiętość 1 = 260. (IFCLENGTHMEASURE) [CENTI METRE]
    Rozpiętość 2 = 260. (IFCLENGTHMEASURE) [CENTI METRE]
    Rozpiętość blachy = 270. (IFCLENGTHMEASURE) [CENTI METRE]
    Szerokość = 270. (IFCLENGTHMEASURE) [CENTI METRE]
    Wysokość blachy = 8. (IFCLENGTHMEASURE) [CENTI METRE]
  Dimensions | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Area = 15.0485987203959 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.01400000000002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Długość = 260. (IFCLENGTHMEASURE) [CENTI METRE]
    Grubość_Modułu = 14.9999999999977 (IFCLENGTHMEASURE) [CENTI METRE]
    Szerokość = 260. (IFCLENGTHMEASURE) [CENTI METRE]
  Dimensions | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Area = 18.8075059130062 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0202613197867011 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions: 926 more contents on 5257 objects not shown
  Constraints | properties | on 1181 objects (1172 IFCBUILDINGELEMENTPROXY, 9 IFCOPENINGELEMENT) | on 2 type objects
    Default Elevation = 260. (IFCLENGTHMEASURE) [CENTI METRE]
  Constraints | properties | on 1004 objects (1004 IFCOPENINGELEMENT)
    Elevation = 49.9 (IFCLENGTHMEASURE) [CENTI METRE]
    Level = "Level: 100 rz. 0.00 - Parter" (IFCLABEL)
  Constraints | properties | on 669 objects (669 IFCBUILDINGELEMENTPROXY)
    Level = "Level: 100 rz. 0.00 - Parter" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 632 objects (439 IFCFLOWTERMINAL, 172 IFCMEMBER, 21 IFCPLATE)
    Level = "Level: 100 rz. 0.00 - Parter" (IFCLABEL)
  Constraints | properties | on 602 objects (437 IFCBUILDINGELEMENTPROXY, 165 IFCFLOWTERMINAL)
    Elevation = 730. (IFCLENGTHMEASURE) [CENTI METRE]
    Host = "<not associated>" (IFCTEXT)
    Level = "Level: 100 rz. 0.00 - Parter" (IFCLABEL)
  Constraints | properties | on 474 objects (411 IFCBUILDINGELEMENTPROXY, 63 IFCOPENINGELEMENT)
    Default Elevation = 360. (IFCLENGTHMEASURE) [CENTI METRE]
  Constraints | properties | on 405 objects (405 IFCBUILDINGELEMENTPROXY)
    Elevation = 1104.00000000009 (IFCLENGTHMEASURE) [CENTI METRE]
    Host = "<not associated>" (IFCTEXT)
    Level = "Level: 099 rz. -374" (IFCLABEL)
  Constraints | properties | on 342 objects (342 IFCBUILDINGELEMENTPROXY)
    Elevation = 1104.00000000008 (IFCLENGTHMEASURE) [CENTI METRE]
    Host = "<not associated>" (IFCTEXT)
    Level = "Level: 099 rz. -374" (IFCLABEL)
  Constraints: 455 more contents on 3219 objects not shown
  Phasing | properties | on 6072 objects (2877 IFCBUILDINGELEMENTPROXY, 1462 IFCOPENINGELEMENT, 715 IFCFLOWTERMINAL, 520 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 565 objects (520 IFCWALLSTANDARDCASE, 26 IFCCURTAINWALL, 10 IFCWALL, 9 IFCOPENINGELEMENT)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Structural | properties | on 68 objects (68 IFCSLAB)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
  Structural | properties | on 3 objects (3 IFCSTAIR)
    Rebar Cover = "Rebar Cover Settings: Rebar Cover 1" (IFCLABEL)
  Structural | properties | on 1 object (1 IFCBEAM)
    A = 0.00572 (IFCAREAMEASURE) [SQUARE_METRE]
    Ix = 4100. (IFCREAL)
    M = 44.9 (IFCREAL)
    Section Shape = 0 (IFCINTEGER)
    W = 0. (IFCREAL)
    Wysokość nominalna = "203" (IFCTEXT)
    Zx = 410. (IFCREAL)
  Structural | properties | on 1 object (1 IFCBEAM)
    Cut Length = 4780. (IFCLENGTHMEASURE) [CENTI METRE]
    Enable Analytical Model = TRUE (IFCBOOLEAN)
    Stick Symbol Location = "Center of Geometry" (IFCIDENTIFIER)
    Structural Usage = "Other" (IFCIDENTIFIER)
  Visibility | properties | on 701 objects (670 IFCBUILDINGELEMENTPROXY, 22 IFCFLOWTERMINAL, 9 IFCOPENINGELEMENT)
    widoczność = TRUE (IFCBOOLEAN)
  Visibility | properties | on 403 objects (403 IFCBUILDINGELEMENTPROXY)
    Obecność 2 = TRUE (IFCBOOLEAN)
    Obecność = TRUE (IFCBOOLEAN)
  Visibility | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    2 stronny = FALSE (IFCBOOLEAN)
    4 stronny = TRUE (IFCBOOLEAN)
  Visibility | properties | on 157 objects (157 IFCBUILDINGELEMENTPROXY)
    2 stronny = TRUE (IFCBOOLEAN)
    4 stronny = FALSE (IFCBOOLEAN)
  Visibility | properties | on 42 objects (31 IFCDOOR, 11 IFCOPENINGELEMENT)
    Supraporta ex = TRUE (IFCBOOLEAN)
    Supraporta in = TRUE (IFCBOOLEAN)
  Visibility | properties | on 13 objects (7 IFCOPENINGELEMENT, 6 IFCBUILDINGELEMENTPROXY)
    Wersja 1 = FALSE (IFCBOOLEAN)
    Wersja 2 = TRUE (IFCBOOLEAN)
    Wersja 2 szafa L = FALSE (IFCBOOLEAN)
    Wersja 2 szafa P = FALSE (IFCBOOLEAN)
  Visibility | properties | on 10 objects (5 IFCBUILDINGELEMENTPROXY, 5 IFCOPENINGELEMENT)
    Wersja 1 = FALSE (IFCBOOLEAN)
    Wersja 2 = TRUE (IFCBOOLEAN)
    Wersja 2 szafa L = TRUE (IFCBOOLEAN)
    Wersja 2 szafa P = TRUE (IFCBOOLEAN)
  Visibility | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Obecność 2 = FALSE (IFCBOOLEAN)
    Obecność = FALSE (IFCBOOLEAN)
  Visibility: 16 more contents on 14 objects not shown
  Pset_WallCommon | properties | on 38 objects (37 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SW1 - żelbet barwiony 40 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 36 objects (36 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 29 objects (25 IFCWALLSTANDARDCASE, 4 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SW4 - bloczki silikatowe tynkowane 18 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 25 objects (25 IFCWALLSTANDARDCASE)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SZ4 - Ocieplenie 18cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 25 objects (25 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Bronze 0.8 mm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 24 objects (24 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    FireRating = "" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SW1 (SZ3) - żelbet barwiony 15 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 21 objects (20 IFCWALLSTANDARDCASE, 1 IFCWALL)
    ExtendToStructure = TRUE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SW1 - żelbet barwiony 20 cm" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 21 objects (21 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "SK1 - Sciana kurtynowa przesła środkowe 2" (IFCIDENTIFIER)
  Pset_WallCommon: 56 more contents on 311 objects not shown
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST - Płyta na gruncie - płyta żelbetowa korekta 18 cm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 8 objects (8 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST - Krata wemna 3 cm" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "S0 - Płyty Placu Gwardii 120 x 120" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 6 objects (6 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST3 - Płyta na gruncie - w.wykonczeniowe korekta" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 5 objects (5 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST7 - Strop między piętrami - w.wykonczeniowe" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 5 objects (5 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST9 - Strop między piętrami biura - w.wykonczeniowe" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "S0 - Płyty Placu Gwardii 120 x 120 ryflowane" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "ST2 - Płyta na gruncie - w.wykonczeniowe korekta" (IFCIDENTIFIER)
  Pset_SlabCommon: 16 more contents on 25 objects not shown
  Materials and Finishes | properties | on 411 objects (411 IFCBUILDINGELEMENTPROXY)
    Materiał = "Beton Barwiony Konstrukcja" (IFCLABEL)
  Materials and Finishes | properties | on 342 objects (342 IFCBUILDINGELEMENTPROXY)
    Materiał = "Akustyka" (IFCLABEL)
  Materials and Finishes | properties | on 249 objects (249 IFCMEMBER)
    Material = "Metal - Aluminum" (IFCLABEL)
  Materials and Finishes | properties | on 46 objects (23 IFCBUILDINGELEMENTPROXY, 23 IFCOPENINGELEMENT)
    Materiał = "Metal - Bronze" (IFCLABEL)
  Materials and Finishes | properties | on 37 objects (21 IFCOPENINGELEMENT, 16 IFCBUILDINGELEMENTPROXY)
    Materiał_Obudowy_Portalu = "Metal - Bronze" (IFCLABEL)
  Materials and Finishes | properties | on 27 objects (27 IFCOPENINGELEMENT)
    Materiał = "Copper bez podziału" (IFCLABEL)
  Materials and Finishes | properties | on 19 objects (19 IFCSLAB) | on 4 type objects
    Structural Material = "Beton Konstrukcja" (IFCLABEL)
  Materials and Finishes | properties | on 14 objects (12 IFCDOOR, 2 IFCOPENINGELEMENT)
    Frame Material = "drewniane" (IFCTEXT)
  Materials and Finishes: 33 more contents on 119 objects not shown
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100 x 2100 SM" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100 x 2100 blokada wc" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 6 objects (6 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100 x 2100" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 5 objects (5 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1140 x 2400 zewn" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100 x 2100 Ra32" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "1000 x 200 Ra37" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1175 x 2400 + 4800 sp" (IFCIDENTIFIER)
  Pset_DoorCommon | properties | on 2 objects (2 IFCDOOR)
    FireRating = "-" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1100 x 2100 KT" (IFCIDENTIFIER)
  Pset_DoorCommon: 26 more contents on 34 objects not shown
  Pset_CurtainWallCommon | properties | on 7 objects (7 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK4 - Barierka podział 120 cm" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 6 objects (6 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 5 objects (5 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK6 - Sciana kurtynowa profilowa wnętrza" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK1 - Sciana kurtynowa przesła środkowe 2" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 2 objects (2 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK4 - Sciana kurtynowa wnętrza pusta" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK5_Podkonstrukcja" (IFCIDENTIFIER)
  Pset_CurtainWallCommon | properties | on 1 object (1 IFCCURTAINWALL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "SK1 - Sciana kurtynowa przesła środkowe 2 z drzwiami 2 ROZW" (IFCIDENTIFIER)
  Pset_MemberCommon | properties | on 29 objects (29 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "60mm x 150mm" (IFCIDENTIFIER)
    Span = 240.000000000018 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 27 objects (27 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50mm x 340mm" (IFCIDENTIFIER)
    Span = 112.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 27 objects (27 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50mm x 340mm" (IFCIDENTIFIER)
    Span = 115. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 25 objects (25 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "60mm x 150mm" (IFCIDENTIFIER)
    Span = 114. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 13 objects (13 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50mm x 340mm" (IFCIDENTIFIER)
    Span = 239.999999999972 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 13 objects (13 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50mm x 340mm" (IFCIDENTIFIER)
    Span = 490.000000000015 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50mm x 340mm" (IFCIDENTIFIER)
    Span = 240. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon | properties | on 11 objects (11 IFCMEMBER)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "50mm x 340mm" (IFCIDENTIFIER)
    Span = 489.999999999922 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_MemberCommon: 40 more contents on 102 objects not shown
  Horizontal Grid | properties | on 30 objects (26 IFCCURTAINWALL, 4 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Horizontal Grid | properties | on 2 type objects
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 240. (IFCLENGTHMEASURE) [CENTI METRE]
  Horizontal Grid | properties | on 2 type objects
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 120. (IFCLENGTHMEASURE) [CENTI METRE]
  Horizontal Grid | properties | on 2 type objects
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 2000. (IFCLENGTHMEASURE) [CENTI METRE]
  Horizontal Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Vertical Grid | properties | on 20 objects (17 IFCCURTAINWALL, 3 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 4 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 4 objects (4 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 1 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 3 objects (3 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 2 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 2 objects (1 IFCCURTAINWALL, 1 IFCOPENINGELEMENT)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 8 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 1 object (1 IFCCURTAINWALL)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Justification = "Beginning" (IFCIDENTIFIER)
    Number = 5 (IFCINTEGER)
    Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 4 type objects
    Adjust for Mullion Size = TRUE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 120. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
    Spacing = 120. (IFCLENGTHMEASURE) [CENTI METRE]
  Vertical Grid | properties | on 1 type object
    Adjust for Mullion Size = FALSE (IFCBOOLEAN)
    Layout = "None" (IFCIDENTIFIER)
  Vertical Grid: 1 more content on 0 objects not shown
  Slab Shape Edit | properties | on 1 object (1 IFCSLAB)
    Curved Edge Condition = 0 (IFCINTEGER)
  Graphics | properties | on 41 objects (36 IFCSLAB, 5 IFCCOVERING) | on 41 type objects
    Coarse Scale Fill Color = 0 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics | properties | on 26 objects (26 IFCSLAB) | on 5 type objects
    Coarse Scale Fill Color = 12632256 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics | properties | on 14 objects (14 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Dash dot" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle1: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 11 objects (11 IFCCOVERING)
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Graphics | properties | on 6 objects (6 IFCSLAB)
    Coarse Scale Fill Color = 8421504 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics | properties | on 3 objects (3 IFCSTAIR)
    Cut Mark Type = "Stair Cut Mark: Single Zigzag" (IFCLABEL)
  Graphics | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    Center Mark Visible = FALSE (IFCBOOLEAN)
  Graphics | properties | on 2 type objects
    Coarse Scale Fill Color = 4144959 (IFCINTEGER)
    Coarse Scale Fill Pattern = "Solid fill" (IFCLABEL)
  Graphics: 1 more content on 0 objects not shown
  Top Rail | properties | on 9 objects (9 IFCRAILING)
    Height = 121.92 (IFCLENGTHMEASURE) [CENTI METRE]
  Handrail 2 | properties | on 9 objects (9 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Handrail 1 | properties | on 9 objects (9 IFCRAILING)
    Position = "None" (IFCIDENTIFIER)
  Construction | properties | on 118 objects (118 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Profile = "System Mullion Profile: Rectangular" (IFCLABEL)
    Thickness = 34. (IFCLENGTHMEASURE) [CENTI METRE]
  Construction | properties | on 79 objects (79 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Profile = "System Mullion Profile: Rectangular" (IFCLABEL)
    Thickness = 15. (IFCLENGTHMEASURE) [CENTI METRE]
  Construction | properties | on 27 objects (27 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Thickness = 15. (IFCLENGTHMEASURE) [CENTI METRE]
  Construction | properties | on 23 objects (23 IFCOPENINGELEMENT)
    Profile = "Szczelina: Szczelina 10 x 30 cm" (IFCLABEL)
  Construction | properties | on 17 objects (17 IFCOPENINGELEMENT)
    Profile = "Szczelina: Szczelina 2 x 25 cm" (IFCLABEL)
  Construction | properties | on 17 objects (17 IFCOPENINGELEMENT)
    Profile = "Szczelina: Szczelina 6 x 10 cm" (IFCLABEL)
  Construction | properties | on 17 objects (17 IFCOPENINGELEMENT)
    Profile = "Szczelina: Szczelina 6 x 17.5 cm" (IFCLABEL)
  Construction | properties | on 16 objects (16 IFCMEMBER)
    Corner Mullion = FALSE (IFCBOOLEAN)
    Position = "Perpendicular to Face" (IFCLABEL)
    Thickness = 6.5 (IFCLENGTHMEASURE) [CENTI METRE]
  Construction: 65 more contents on 137 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 623 objects (623 IFCBUILDINGELEMENTPROXY)
    Reference = "tryskacz korytarz" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Reference = "260 x 260" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 337 objects (337 IFCBUILDINGELEMENTPROXY)
    Reference = "260 x 260 cm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 251 objects (251 IFCBUILDINGELEMENTPROXY)
    Reference = "Moduł otwór duży" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 210 objects (210 IFCBUILDINGELEMENTPROXY)
    Reference = "Płaskie" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 178 objects (178 IFCBUILDINGELEMENTPROXY)
    Reference = "Śrecnica 17 cm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 157 objects (157 IFCBUILDINGELEMENTPROXY)
    Reference = "Floorbox 20 x 20 cm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 130 objects (130 IFCBUILDINGELEMENTPROXY)
    Reference = "360 x 130 cm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 50 more contents on 654 objects not shown
  Profile | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Analytical Properties | properties | on 80 objects (68 IFCSLAB, 12 IFCCOVERING) | on 13 type objects
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  Analytical Properties | properties | on 4 objects (4 IFCCOVERING)
    Absorptance = 0.1 (IFCREAL)
    Heat Transfer Coefficient (U) = 51. (IFCREAL)
    Roughness = 1 (IFCINTEGER)
    Thermal Resistance (R) = 0.0196078431372549 (IFCREAL)
    Thermal mass = 10752. (IFCREAL)
  Analytical Properties | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 44 type objects
    Analytic Construction = "<None>" (IFCTEXT)
  Analytical Properties | properties | on 32 type objects
    Absorptance = 0.7 (IFCREAL)
    Roughness = 3 (IFCINTEGER)
  Analytical Properties | properties | on 12 type objects
    Analytic Construction = "Metal" (IFCTEXT)
    Heat Transfer Coefficient (U) = 3.7021 (IFCREAL)
    Solar Heat Gain Coefficient = 0. (IFCREAL)
    Thermal Resistance (R) = 0.270116960643959 (IFCREAL)
    Visual Light Transmittance = 0. (IFCREAL)
  Analytical Properties | properties | on 3 type objects
    Absorptance = 0.7 (IFCREAL)
    Heat Transfer Coefficient (U) = 7720. (IFCREAL)
    Roughness = 3 (IFCINTEGER)
    Thermal Resistance (R) = 0.000129533678756477 (IFCREAL)
    Thermal mass = 172095. (IFCREAL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 30. (IFCCOUNTMEASURE)
    NumberOfTreads = 29. (IFCCOUNTMEASURE)
    Reference = "Schody Monolityczne 17x26" (IFCIDENTIFIER)
    RiserHeight = 17.0689655172379 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Schody Monolityczne 17x26" (IFCIDENTIFIER)
    RiserHeight = 17.0000000000039 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Schody Monolityczne 17x26" (IFCIDENTIFIER)
    RiserHeight = 17.000000000005 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 30. (IFCCOUNTMEASURE)
    NumberOfTreads = 29. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run" (IFCIDENTIFIER)
    RiserHeight = 17.0689655172379 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WaistThickness = 160. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 80. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 2 objects (2 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 22. (IFCCOUNTMEASURE)
    NumberOfTreads = 22. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run" (IFCIDENTIFIER)
    RiserHeight = 17.0000000000039 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WaistThickness = 145. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 72.5 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NosingLength = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 18. (IFCCOUNTMEASURE)
    Reference = "Monolithic Run" (IFCIDENTIFIER)
    RiserHeight = 17.000000000005 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLength = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    TreadLengthAtOffset = 28. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WaistThickness = 160. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    WalkingLineOffset = 80. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 6 objects (6 IFCCOVERING)
    Finish = "Default transparent;Ceiling Tile 600 x 600;" (IFCTEXT)
    Reference = "SKA (60x60 cm)" (IFCIDENTIFIER)
    TotalThickness = 5.2 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    Finish = "Welna Mineralna;Plaster;" (IFCTEXT)
    Reference = "SAK 1" (IFCIDENTIFIER)
    TotalThickness = 5. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    Finish = "Default transparent;Ceiling Tile 600 x 600(1);" (IFCTEXT)
    Reference = "SKA (210x60 cm)" (IFCIDENTIFIER)
    TotalThickness = 5.2 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Default;Ceiling Tile 600 x 1200;" (IFCTEXT)
    Reference = "SGK" (IFCIDENTIFIER)
    TotalThickness = 5.2 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Default;Ceiling Tile 600 x 1200;" (IFCTEXT)
    Reference = "SGKh" (IFCIDENTIFIER)
    TotalThickness = 5.2 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Finish = "Beton Barwiony Konstrukcja;" (IFCTEXT)
    Reference = "SUFIT SBAG" (IFCIDENTIFIER)
    TotalThickness = 15. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Pset_ColumnCommon | properties | on 5 objects (5 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "40 x 40 cm" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "40 x 40 cm" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
  Treads | properties | on 5 objects (5 IFCSTAIRFLIGHT)
    Apply Nosing Profile = "Front Only" (IFCIDENTIFIER)
    Nosing Length = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Tread = FALSE (IFCBOOLEAN)
    Tread Thickness = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  Treads | properties | on 2 objects (2 IFCSLAB)
    Same as Run = TRUE (IFCBOOLEAN)
  Pset_PlateCommon | properties | on 23 objects (23 IFCPLATE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Glazed" (IFCIDENTIFIER)
  Risers | properties | on 5 objects (5 IFCSTAIRFLIGHT)
    Riser = FALSE (IFCBOOLEAN)
    Riser Thickness = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Riser To Tread Connection = "Extend Riser Behind Tread" (IFCIDENTIFIER)
    Slanted = TRUE (IFCBOOLEAN)
  Supports | properties | on 3 objects (3 IFCSTAIR)
    Left Lateral Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Left Support = "None" (IFCIDENTIFIER)
    Middle Support = FALSE (IFCBOOLEAN)
    Middle Support Number = 0 (IFCINTEGER)
    Right Lateral Offset = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Right Support = "None" (IFCIDENTIFIER)
  Calculation Rules | properties | on 3 objects (3 IFCSTAIR)
    Maximum Riser Height = 17. (IFCLENGTHMEASURE) [CENTI METRE]
    Minimum Run Width = 145. (IFCLENGTHMEASURE) [CENTI METRE]
    Minimum Tread Depth = 26. (IFCLENGTHMEASURE) [CENTI METRE]
  Pset_DistributionFlowElementCommon | properties | on 279 objects (279 IFCFLOWTERMINAL)
    Reference = "TRIL 20.1030.25 116mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 128 objects (128 IFCFLOWTERMINAL)
    Reference = "MWP_M_I-VALO ZETA 380mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 86 objects (86 IFCFLOWTERMINAL)
    Reference = "MWP_M_Ray Pendant" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 47 objects (47 IFCFLOWTERMINAL)
    Reference = "MODULES LED COB 3000K 230V 1470lm 13.5W CRI 90" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 42 objects (42 IFCFLOWTERMINAL)
    Reference = "Pleiad Comfort G3 183 mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 26 objects (26 IFCFLOWTERMINAL)
    Reference = "TRIL 20.1030.35 116mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 21 objects (21 IFCFLOWTERMINAL)
    Reference = "oświetlenie awaryjne D1W" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 17 objects (17 IFCFLOWTERMINAL)
    Reference = "Pleiad Comfort G3 110 mm" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon: 10 more contents on 69 objects not shown
  Electrical - Circuiting | properties | on 368 objects (368 IFCFLOWTERMINAL)
    Electrical Data = "230 V/1-60 VA" (IFCTEXT)
  Electrical - Circuiting | properties | on 71 objects (71 IFCFLOWTERMINAL)
    Electrical Data = "120 V/1-60 VA" (IFCTEXT)
  Electrical - Circuiting | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Supply From = "" (IFCTEXT)
  Electrical - Lighting | properties | on 714 objects (714 IFCFLOWTERMINAL)
    Calculate Coefficient of Utilization = FALSE (IFCBOOLEAN)
  Electrical - Loads | properties | on 685 objects (685 IFCFLOWTERMINAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Electrical - Loads | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Apparent Load Phase A = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase B = 0. (IFCPOWERMEASURE) [WATT]
    Apparent Load Phase C = 0. (IFCPOWERMEASURE) [WATT]
    Total Connected = 0. (IFCPOWERMEASURE) [WATT]
    Total Demand Factor = 1. (IFCREAL)
    Total Estimated Demand = 0. (IFCPOWERMEASURE) [WATT]
  Electrical - Loads | properties | on 11 type objects
    Apparent Load = 60. (IFCPOWERMEASURE) [WATT]
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HEB_120x120" (IFCIDENTIFIER)
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 4780. (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
  Geometric Position | properties | on 1 object (1 IFCBEAM)
    End Extension = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    Join Status = "Both joins enabled" (IFCIDENTIFIER)
    Start Extension = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    y Justification = "Origin" (IFCIDENTIFIER)
    y Offset Value = 0. (IFCLENGTHMEASURE) [CENTI METRE]
    yz Justification = "Uniform" (IFCIDENTIFIER)
    z Justification = "Top" (IFCIDENTIFIER)
    z Offset Value = 0. (IFCLENGTHMEASURE) [CENTI METRE]
  General | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Location = "Sala wystaw czasowych 1.25" (IFCTEXT)
  Pset_RailingCommon | properties | on 7 objects (7 IFCRAILING)
    Height = 121.92 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Prostokątna wąska 15cm" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 121.92 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Pełna policzkowa biegi" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 1 object (1 IFCRAILING)
    Height = 121.92 (IFCPOSITIVELENGTHMEASURE) [CENTI METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Pełna policzkowa szpoczniki" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 14 objects (14 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 14 (IFCINTEGER)
  Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100 KT:677092 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe supraporta 2str:1200 x 2100:677229 | predefined | on 2 type objects
  Green Building Properties | properties | on 19 type objects
    Wsp. U = "-" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Wsp. U = "1,1" (IFCTEXT)
  Drzwi stalowe 1skrz blokowe:1200 x 2400 brąz:677510 | predefined | on 2 type objects
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 50mm x 65mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50mm x 65mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 60mm x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 60mm x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 60mm x 150mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 80mm x 200mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 50mm x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50mm x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50mm x 150mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 117mm x 300mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
  Horizontal Mullions | properties | on 1 type object
    Interior Type = "Rectangular Mullion: 50mm x 65mm" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50mm x 340mm" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 60mm x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 60mm x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 60mm x 150mm" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: C 200 Right" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: C 200 Left" (IFCLABEL)
    Interior Type = "Rectangular Mullion: HEB 200" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 50mm x 150mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 50mm x 150mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 50mm x 150mm" (IFCLABEL)
  Vertical Mullions | properties | on 1 type object
    Border 1 Type = "Rectangular Mullion: 117mm x 300mm" (IFCLABEL)
    Border 2 Type = "Rectangular Mullion: 117mm x 300mm" (IFCLABEL)
    Interior Type = "Rectangular Mullion: 40mm x 80mm" (IFCLABEL)
  Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100:1462375 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe supraporta 2str:1100 x 2100:1462378 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1200 x 2400 beton EI-30:2620844 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra32 KD2:2849913 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra27:3273618 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:3273632 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe supraporta 1str:1100 x 2100:3276145 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1100 x 2100 Ra32 KD2:3389960 | predefined | on 2 type objects
  Drzwi stalowe 2skrz niesym blokowe:1900 x 2400 (podział 110 80) ap beton poprawione:4071345 | predefined | on 2 type objects
  Electrical | properties | on 6 type objects
    Ballast Number of Poles = 1 (IFCINTEGER)
    Ballast Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Lamp = "A-19" (IFCTEXT)
    Load Classification = "Lighting - Dwelling Unit" (IFCLABEL)
    Wattage Comments = "" (IFCTEXT)
  Electrical | properties | on 5 type objects
    Ballast Number of Poles = 1 (IFCINTEGER)
    Ballast Voltage = 120. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Lamp = "A-19" (IFCTEXT)
    Load Classification = "Lighting - Dwelling Unit" (IFCLABEL)
    Wattage Comments = "" (IFCTEXT)
  Photometrics | properties | on 11 type objects
    Ballast Loss = 1. (IFCREAL)
    Color Filter = 16777215 (IFCINTEGER)
    Dimming Lamp Color Temperature Shift = "<None>" (IFCIDENTIFIER)
    Efficacy = 14.25 (IFCREAL) [derived "Luminous Efficacy"]
    Illuminance = 1230.85393087727 (IFCILLUMINANCEMEASURE) [LUX]
    Initial Color = 0 (IFCINTEGER)
    Initial Color Temperature = 2800. (IFCREAL) [KELVIN]
    Initial Intensity = 0 (IFCINTEGER)
    Lamp Lumen Depreciation = 1. (IFCREAL)
    Lamp Tilt Loss = 1. (IFCREAL)
    Light Loss Factor = 0 (IFCINTEGER)
    Light Source Definition (family) = "Point+Spot" (IFCTEXT)
    Luminaire Dirt Depreciation = 1. (IFCREAL)
    Luminous Flux = 3420. (IFCLUMINOUSFLUXMEASURE) [LUMEN]
    Luminous Intensity = 11435.0071974448 (IFCLUMINOUSINTENSITYMEASURE) [CANDELA]
    Spot Beam Angle = 30. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Spot Field Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Surface Depreciation Loss = 1. (IFCREAL)
    Temperature Loss = 1. (IFCREAL)
    Tilt Angle = 90. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Total Light Loss Factor = 1. (IFCREAL)
    Voltage Loss = 1. (IFCREAL)
    Wattage = 240. (IFCPOWERMEASURE) [WATT]
  Drzwi stalowe 2skrz niesym blokowe:1900 x 2400 mm (podział 110 80) EI-30 ap beton poprawione:7117541 | predefined | on 2 type objects
  Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7133277 | predefined | on 2 type objects
  Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7137746 | predefined | on 2 type objects
  Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7137829 | predefined | on 2 type objects
  Drzwi indywidualne SWC blokowe:1175 x 2400 + 4800 sp:7138385 | predefined | on 2 type objects
  Drzwi indywidualne SWC blokowe:3275 x 7150 + 50 sp:7138557 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1100 x 2400 (beton):7898971 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1100 x 2100:8563773 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2200 x 2375 ap:9120566 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2150 x 2375 ap:9120568 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2200 x 2375 ap EZ:9120569 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2155 x 2375 ap:9120572 | predefined | on 2 type objects
  Drzwi szklane 2skrz:1900 x 2400 (120-70) ap:9121792 | predefined | on 2 type objects
  Drzwi szklane 1skrz:1100 x 2400 Ra37:9125870 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2200 x 2400 Ei-30 Ra32:9126746 | predefined | on 2 type objects
  Drzwi szklane 1skrz:1180 x 2400 EI-30:9132033 | predefined | on 2 type objects
  Drzwi szklane przesuwne:2400 X 2400:9182862 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe supraporta 1str:1100 x 2100:9761979 | predefined | on 2 type objects
  Drzwi szklane 1skrz:1100 x 2400 Ra37:9762805 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1200 x 2400 brąz:9789241 | predefined | on 2 type objects
  Drzwi indywidualne SWC Z:1200 x 2400:10012380 | predefined | on 2 type objects
  Drzwi indywidualne SWC P:1700 x 7300:10014261 | predefined | on 2 type objects
  Drzwi drewniane 2skrz blokowe supraporta 2str:1600 x 2100 (110-50) EI-30 KD1:10537732 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2142 x 2375 ap fasada rozwieralna:13254295 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:1226310 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1200 x 2100:1226311 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:1226312 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:1226313 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:1226320 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:2784990 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe szklane SP:1100 x 2100 Ra32:5624212 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:0900 x 2100:8053159 | predefined | on 2 type objects
  Drzwi szklane 2skrz:1600 x 2400 (110-50) EI-30:9126849 | predefined | on 2 type objects
  Drzwi szklane 2skrz:2200 X 2400 zewn:9126955 | predefined | on 2 type objects
  Drzwi szklane 1skrz:1140 x 2400 zewn:9129254 | predefined | on 2 type objects
  Drzwi szklane 1skrz:1100 x 2400 Ra32:9132676 | predefined | on 2 type objects
  Drzwi szklane 1skrz:1100 x 2400 Ra32:9132692 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:9768762 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:9768765 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:9768768 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 blokada wc:9768769 | predefined | on 2 type objects
  Drzwi drewniane 1skrz blokowe:1100 x 2100 SM:10045917 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1000 x 200 Ra37:5941210 | predefined | on 2 type objects
  Drzwi stalowe 1skrz blokowe:1000 x 200 Ra37:5941281 | predefined | on 2 type objects